{
  "version": 1,
  "minor_version": 1,
  "key": "bluetooth.passive_update_processor",
  "data": {
    "01K0E2PJYPJ8GQHS134XXM8BYV": {
      "binary_sensor": {
        "devices": {
          "": {
            "name": "Plant Sensor 17A3",
            "manufacturer": "Xiaomi",
            "model": "HHCCJCY01"
          }
        },
        "entity_descriptions": {},
        "entity_names": {},
        "entity_data": {}
      },
      "sensor": {
        "devices": {
          "": {
            "name": "Plant Sensor 17A3",
            "manufacturer": "Xiaomi",
            "model": "HHCCJCY01"
          }
        },
        "entity_descriptions": {
          "moisture___": {
            "key": "moisture_%",
            "device_class": "moisture",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "signal_strength___": {
            "key": "signal_strength_dBm",
            "device_class": "signal_strength",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "native_unit_of_measurement": "dBm",
            "state_class": "measurement"
          },
          "battery___": {
            "key": "battery_%",
            "device_class": "battery",
            "entity_category": "diagnostic",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "conductivity___": {
            "key": "µS/cm",
            "device_class": "conductivity",
            "native_unit_of_measurement": "μS/cm",
            "state_class": "measurement"
          },
          "temperature___": {
            "key": "temperature_°C",
            "device_class": "temperature",
            "native_unit_of_measurement": "°C",
            "state_class": "measurement"
          },
          "illuminance___": {
            "key": "illuminance_lx",
            "device_class": "illuminance",
            "native_unit_of_measurement": "lx",
            "state_class": "measurement"
          }
        },
        "entity_names": {},
        "entity_data": {
          "moisture___": 13,
          "signal_strength___": -57,
          "battery___": 21,
          "conductivity___": 187,
          "temperature___": 18.9,
          "illuminance___": 526
        }
      }
    },
    "01KB0CKC2PVKFYG3M5CCH2D1S1": {
      "binary_sensor": {
        "devices": {
          "": {
            "name": "SBBT-EUa3bb A3BB",
            "model": "BTHome sensor"
          }
        },
        "entity_descriptions": {},
        "entity_names": {},
        "entity_data": {}
      },
      "sensor": {
        "devices": {
          "": {
            "name": "SBBT-EUa3bb A3BB",
            "model": "BTHome sensor"
          }
        },
        "entity_descriptions": {
          "packet_id___": {
            "key": "packet_id",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "translation_key": "packet_id",
            "state_class": "measurement"
          },
          "battery___": {
            "key": "battery_%",
            "device_class": "battery",
            "entity_category": "diagnostic",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "signal_strength___": {
            "key": "signal_strength_dBm",
            "device_class": "signal_strength",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "native_unit_of_measurement": "dBm",
            "state_class": "measurement"
          }
        },
        "entity_names": {
          "packet_id___": "Packet Id",
          "battery___": "Battery",
          "signal_strength___": "Signal Strength"
        },
        "entity_data": {
          "packet_id___": 69,
          "battery___": 100,
          "signal_strength___": -68
        }
      }
    },
    "01JKJGNAG8GSYBPZ9Q6V8PBBVR": {
      "sensor": {
        "devices": {
          "": {
            "name": "IO Series 6/7 2A7C",
            "manufacturer": "Oral-B",
            "model": "IO Series 6/7"
          }
        },
        "entity_descriptions": {
          "time___": {
            "key": "time",
            "device_class": "duration",
            "native_unit_of_measurement": "s",
            "state_class": "total_increasing"
          },
          "sector___": {
            "key": "sector",
            "device_class": "enum",
            "entity_category": "diagnostic",
            "translation_key": "sector",
            "options": [
              "sector_1",
              "sector_3",
              "sector_2",
              "no_sector",
              "sector_4",
              "success"
            ]
          },
          "number_of_sectors___": {
            "key": "number_of_sectors",
            "entity_category": "diagnostic",
            "translation_key": "number_of_sectors"
          },
          "sector_timer___": {
            "key": "sector_timer",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "translation_key": "sector_timer"
          },
          "toothbrush_state___": {
            "key": "toothbrush_state",
            "device_class": "enum",
            "name": null,
            "translation_key": "toothbrush_state",
            "options": [
              "initializing",
              "sleeping",
              "final_test",
              "idle",
              "unknown",
              "charging",
              "flight_menu",
              "running",
              "off",
              "setup",
              "pcb_test",
              "selection_menu",
              "transport"
            ]
          },
          "pressure___": {
            "key": "pressure",
            "device_class": "enum",
            "translation_key": "pressure",
            "options": [
              "high",
              "low",
              "power_button_pressed",
              "normal",
              "button_pressed"
            ]
          },
          "mode___": {
            "key": "mode",
            "device_class": "enum",
            "entity_category": "diagnostic",
            "translation_key": "mode",
            "options": [
              "gum_care",
              "whitening",
              "settings",
              "intense",
              "daily_clean",
              "unknown",
              "massage",
              "off",
              "whiten",
              "super_sensitive",
              "sensitive",
              "turbo",
              "deep_clean",
              "tongue_cleaning"
            ]
          },
          "signal_strength___": {
            "key": "signal_strength",
            "device_class": "signal_strength",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "native_unit_of_measurement": "dBm",
            "state_class": "measurement"
          },
          "battery_percent___": {
            "key": "battery_percent",
            "device_class": "battery",
            "entity_category": "diagnostic",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          }
        },
        "entity_names": {},
        "entity_data": {
          "time___": 0,
          "sector___": "no sector",
          "number_of_sectors___": 0,
          "sector_timer___": 0,
          "toothbrush_state___": "idle",
          "pressure___": "normal",
          "mode___": "daily clean",
          "signal_strength___": -78,
          "battery_percent___": 49
        }
      }
    },
    "01KEY2RXFY8K8F34ZVX1CR423Q": {
      "binary_sensor": {
        "devices": {
          "": {
            "name": "Shelly BLU H&T F098",
            "manufacturer": "Shelly",
            "model": "BLU H&T"
          }
        },
        "entity_descriptions": {},
        "entity_names": {},
        "entity_data": {}
      },
      "sensor": {
        "devices": {
          "": {
            "name": "Shelly BLU H&T F098",
            "manufacturer": "Shelly",
            "model": "BLU H&T"
          }
        },
        "entity_descriptions": {
          "packet_id___": {
            "key": "packet_id",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "translation_key": "packet_id",
            "state_class": "measurement"
          },
          "battery___": {
            "key": "battery_%",
            "device_class": "battery",
            "entity_category": "diagnostic",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "humidity___": {
            "key": "humidity_%",
            "device_class": "humidity",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "temperature___": {
            "key": "temperature_°C",
            "device_class": "temperature",
            "native_unit_of_measurement": "°C",
            "state_class": "measurement"
          },
          "signal_strength___": {
            "key": "signal_strength_dBm",
            "device_class": "signal_strength",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "native_unit_of_measurement": "dBm",
            "state_class": "measurement"
          }
        },
        "entity_names": {},
        "entity_data": {
          "packet_id___": 228,
          "battery___": 98,
          "humidity___": 46,
          "temperature___": 19.7,
          "signal_strength___": -39
        }
      }
    },
    "01KEWRRP9CQC24R82T5AE0N3BF": {
      "binary_sensor": {
        "devices": {
          "": {
            "name": "SBTR-EU4718 4718",
            "model": "BTHome sensor"
          }
        },
        "entity_descriptions": {},
        "entity_names": {},
        "entity_data": {}
      },
      "sensor": {
        "devices": {
          "": {
            "name": "SBTR-EU4718 4718",
            "model": "BTHome sensor"
          }
        },
        "entity_descriptions": {
          "packet_id___": {
            "key": "packet_id",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "translation_key": "packet_id",
            "state_class": "measurement"
          },
          "battery___": {
            "key": "battery_%",
            "device_class": "battery",
            "entity_category": "diagnostic",
            "native_unit_of_measurement": "%",
            "state_class": "measurement"
          },
          "temperature_1___": {
            "key": "temperature_°C",
            "device_class": "temperature",
            "native_unit_of_measurement": "°C",
            "state_class": "measurement"
          },
          "temperature_2___": {
            "key": "temperature_°C",
            "device_class": "temperature",
            "native_unit_of_measurement": "°C",
            "state_class": "measurement"
          },
          "raw___": {
            "key": "raw",
            "translation_key": "raw"
          },
          "signal_strength___": {
            "key": "signal_strength_dBm",
            "device_class": "signal_strength",
            "entity_category": "diagnostic",
            "entity_registry_enabled_default": false,
            "native_unit_of_measurement": "dBm",
            "state_class": "measurement"
          },
          "temperature_3___": {
            "key": "temperature_°C",
            "device_class": "temperature",
            "native_unit_of_measurement": "°C",
            "state_class": "measurement"
          }
        },
        "entity_names": {},
        "entity_data": {
          "packet_id___": 34,
          "battery___": 100,
          "temperature_1___": 18.0,
          "temperature_2___": 18.9,
          "raw___": "04",
          "signal_strength___": -48,
          "temperature_3___": 18.7
        }
      }
    }
  }
}