# For more options and information see
# http://rpf.io/configtxt
# Some settings may impact device functionality. See link above for details

# uncomment if you get no picture on HDMI for a default "safe" mode
#hdmi_safe=1

# uncomment this if your display has a black border of unused pixels visible
# and your display can output without overscan
#disable_overscan=1

# uncomment the following to adjust overscan. Use positive numbers if console
# goes off screen, and negative if there is too much border
#overscan_left=16
#overscan_right=16
#overscan_top=16
#overscan_bottom=16

# uncomment to force a console size. By default it will be display's size minus
# overscan.
#framebuffer_width=1280
#framebuffer_height=720

# uncomment if hdmi display is not detected and composite is being output
#hdmi_force_hotplug=1

# uncomment to force a specific HDMI mode (this will force VGA)
#hdmi_group=1
#hdmi_mode=1

# uncomment to force a HDMI mode rather than DVI. This can make audio work in
# DMT (computer monitor) modes
#hdmi_drive=2

# uncomment to increase signal to HDMI, if you have interference, blanking, or
# no display
#config_hdmi_boost=4

# uncomment for composite PAL
#sdtv_mode=2

#uncomment to overclock the arm. 700 MHz is the default.
#arm_freq=800

# Uncomment some or all of these to enable the optional hardware interfaces
#dtparam=i2c_arm=on
#dtparam=i2s=on
dtparam=spi=on

# Uncomment this to enable infrared communication.
#dtoverlay=gpio-ir,gpio_pin=17
#dtoverlay=gpio-ir-tx,gpio_pin=18

# Additional overlays and parameters are documented /boot/overlays/README

# Enable audio (loads snd_bcm2835)
dtparam=audio=on


####################################################
####     MainsailOS specific configurations     ####
####################################################
####      DO NOT CHANGE SECTION BELOW !!!       ####
####   UNLESS YOU KNOW WHAT YOU ARE DOING !!!   ####
####################################################

## For more options and information see
## https://www.raspberrypi.com/documentation/computers/config_txt.html
## Some settings may impact device functionality. See link above for details

## For additional information about device filters see
## https://www.raspberrypi.com/documentation/computers/config_txt.html#model-filters


[pi0]
## This affects Pi Zero(W) and Pi Zero2
## Due lag of RAM, limit GPU RAM
gpu_mem=128

[pi2]
gpu_mem=256

[pi3]
## Use 256 if 1Gb Ram Model!
gpu_mem=128
# gpu_mem=256

[pi4]
## Enable DRM VC4 V3D driver on top of the dispmanx display stack
dtoverlay=vc4-fkms-v3d
max_framebuffers=2
## Do not use more than 256Mb on Pi Model 4, it uses its own Management.
gpu_mem=256

[all]

## SPI Interface is enabled by default for Input Shaper
## To revert that comment out line #48
## This colides with Hyperpixel Display!
## Hyperpixel Screen uses the same Pin for Backlight.

## Enable Hardware UART for Serial Communication
enable_uart=1
dtoverlay=disable-bt

## Enable VideoCore at boot, needed for Raspicams and DSI devices.
start_x=1

### EXPERIMENTAL - Enable 64bit Kernel
### The 64-bit kernel will only work on:
### Raspberry Pi 3, 3+, 4, 400, Zero 2 W and 2B rev 1.2
### and Raspberry Pi Compute Modules 3, 3+ and 4.
# arm_64bit=1

dtoverlay=dwc2,dr_mode=host

####################################################
