(module USB4510_NoPaste (layer F.Cu) (tedit 620C1622)
  (attr smd)
  (fp_text reference REF** (at 0 -3.35) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB4510_NoPaste (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.62 0) (end -4.62 -5.7) (layer Edge.Cuts) (width 0.2))
  (fp_line (start -4.12 -6.2) (end 4.12 -6.2) (layer Edge.Cuts) (width 0.2))
  (fp_line (start 4.62 0) (end 4.62 -5.7) (layer Edge.Cuts) (width 0.2))
  (fp_line (start -4.47 0.5) (end -4.47 -6) (layer F.Fab) (width 0.05))
  (fp_line (start 4.47 0.5) (end 4.47 -6) (layer F.Fab) (width 0.05))
  (fp_line (start -4.47 0.5) (end 4.47 0.5) (layer F.Fab) (width 0.05))
  (fp_line (start 4.47 -6) (end -4.47 -6) (layer F.Fab) (width 0.05))
  (fp_arc (start -4.12 -5.7) (end -4.12 -6.2) (angle -90) (layer Edge.Cuts) (width 0.2))
  (fp_arc (start 4.12 -5.7) (end 4.62 -5.7) (angle -90) (layer Edge.Cuts) (width 0.2))
  (pad S1 thru_hole oval (at 5.62 -5.6) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -5.62 -1.6) (size 1 2.2) (drill oval 0.6 1.8) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at 5.62 -1.6) (size 1 2.2) (drill oval 0.6 1.8) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at -5.62 -5.6) (size 1 1.8) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
  (pad A1 smd rect (at -3.2 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad A4 smd rect (at -2.4 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad B12 smd rect (at -3.2 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad B9 smd rect (at -2.4 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad B8 smd rect (at -1.75 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad A5 smd rect (at -1.25 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad B7 smd rect (at -0.75 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad A6 smd rect (at -0.25 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad A7 smd rect (at 0.25 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad B6 smd rect (at 0.75 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad A8 smd rect (at 1.25 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad B5 smd rect (at 1.75 -6.75) (size 0.3 1.1) (layers F.Cu F.Mask))
  (pad A9 smd rect (at 2.4 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad B4 smd rect (at 2.4 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad B1 smd rect (at 3.2 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (pad A12 smd rect (at 3.2 -6.75) (size 0.6 1.1) (layers F.Cu F.Mask))
  (model ${KIPRJMOD}/../lib/GCT_USB.3dshapes/proprietary/USB4510-03-1-A.stp
    (offset (xyz 0 -0.5 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
