(module SolderPads_2mm_3_STRAIN (layer F.Cu) (tedit 622E2DE5)
  (attr virtual)
  (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SolderPads_2mm_3_STRAIN (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1 -1.5) (end -1 -1) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.5 -1.5) (end -1 -1.5) (layer F.SilkS) (width 0.15))
  (fp_text user + (at 0 2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user - (at 4 2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %V (at 2 2.5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd oval (at 0 0) (size 1.25 2.5) (layers F.Cu F.Mask))
  (pad 2 smd oval (at 2 0) (size 1.25 2.5) (layers F.Cu F.Mask))
  (pad 3 smd oval (at 4 0) (size 1.25 2.5) (layers F.Cu F.Mask))
)
