(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~90~ubuntu20.04.1)

  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 84)
    (zones 0)
    (modules 3)
    (nets 29)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.18)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 /P27)
  (net 2 "Net-(J1-Pad13)")
  (net 3 "Net-(J1-Pad12)")
  (net 4 "Net-(J1-Pad11)")
  (net 5 "Net-(J1-Pad10)")
  (net 6 "Net-(J1-Pad9)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad6)")
  (net 10 "Net-(J1-Pad5)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad2)")
  (net 14 /P25)
  (net 15 /P28)
  (net 16 "Net-(J2-Pad13)")
  (net 17 "Net-(J2-Pad12)")
  (net 18 "Net-(J2-Pad11)")
  (net 19 "Net-(J2-Pad10)")
  (net 20 "Net-(J2-Pad9)")
  (net 21 "Net-(J2-Pad8)")
  (net 22 "Net-(J2-Pad7)")
  (net 23 "Net-(J2-Pad6)")
  (net 24 "Net-(J2-Pad5)")
  (net 25 "Net-(J2-Pad4)")
  (net 26 "Net-(J2-Pad3)")
  (net 27 "Net-(J2-Pad2)")
  (net 28 /P26)

  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.18)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /P25)
    (add_net /P26)
    (add_net /P27)
    (add_net /P28)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
  )

  (module BM28:BM28B0.6-24DS (layer F.Cu) (tedit 6180705A) (tstamp 61814D44)
    (at 74.93 62.23)
    (path /61B58607)
    (attr smd)
    (fp_text reference J3 (at -3.515 0 90) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_02x14_Odd_Even (at 0 3.6) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 28 smd rect (at 0.745 2.63) (size 0.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 15 /P28))
    (pad 27 smd rect (at -0.745 2.63) (size 0.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 /P27))
    (pad 26 smd rect (at 0.745 -2.63) (size 0.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 28 /P26))
    (pad 25 smd rect (at -0.745 -2.63) (size 0.31 0.53) (layers F.Cu F.Paste F.Mask)
      (net 14 /P25))
    (pad 24 smd rect (at 0.795 1.925) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad13)"))
    (pad 23 smd rect (at -0.795 1.925) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad13)"))
    (pad 22 smd rect (at 0.795 1.575) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad12)"))
    (pad 21 smd rect (at -0.795 1.575) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad12)"))
    (pad 20 smd rect (at 0.795 1.225) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad11)"))
    (pad 19 smd rect (at -0.795 1.225) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad11)"))
    (pad 18 smd rect (at 0.795 0.875) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-Pad10)"))
    (pad 17 smd rect (at -0.795 0.875) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 16 smd rect (at 0.795 0.525) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-Pad9)"))
    (pad 15 smd rect (at -0.795 0.525) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad9)"))
    (pad 14 smd rect (at 0.795 0.175) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 13 smd rect (at -0.795 0.175) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 12 smd rect (at 0.795 -0.175) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J2-Pad7)"))
    (pad 11 smd rect (at -0.795 -0.175) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 10 smd rect (at 0.795 -0.525) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 9 smd rect (at -0.795 -0.525) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 8 smd rect (at 0.795 -0.875) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 7 smd rect (at -0.795 -0.875) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0.795 -1.225) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -0.795 -1.225) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 4 smd rect (at 0.795 -1.575) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-Pad3)"))
    (pad 3 smd rect (at -0.795 -1.575) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.795 -1.925) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -0.795 -1.925) (size 0.41 0.18) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad2)"))
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 61814D24)
    (at 81.28 45.72 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (path /61B5ADB8)
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x14_Male (at 0 -35.35) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -34.29) (end -1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -34.29) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.33 -34.35) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 1.8) (end -1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -34.8) (end 1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -34.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /P28))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /P26))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC) (tstamp 61814D02)
    (at 68.58 45.72 180)
    (descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x14 2.54mm single row")
    (path /61B59B74)
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text value Conn_01x14_Male (at 0 -35.35) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_text user %R (at 0 -16.51 270) (layer B.Fab)
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    )
    (fp_line (start -0.635 1.27) (end 1.27 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 1.27) (end 1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start 1.27 -34.29) (end -1.27 -34.29) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 -34.29) (end -1.27 0.635) (layer B.Fab) (width 0.1))
    (fp_line (start -1.27 0.635) (end -0.635 1.27) (layer B.Fab) (width 0.1))
    (fp_line (start -1.33 -34.35) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end -1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start 1.33 -1.27) (end 1.33 -34.35) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.27) (end 1.33 -1.27) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.33 1.33) (end 0 1.33) (layer B.SilkS) (width 0.12))
    (fp_line (start -1.8 1.8) (end -1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start -1.8 -34.8) (end 1.8 -34.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 -34.8) (end 1.8 1.8) (layer B.CrtYd) (width 0.05))
    (fp_line (start 1.8 1.8) (end -1.8 1.8) (layer B.CrtYd) (width 0.05))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /P27))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /P25))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_text BM28B0.6-24DS (at 74.93 58.42 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify left))
  )
  (gr_text 16 (at 78.74 66.04) (layer F.SilkS) (tstamp 61816215)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 6 (at 78.74 53.34) (layer F.SilkS) (tstamp 61816214)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 22 (at 78.74 73.66) (layer F.SilkS) (tstamp 61816213)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 8 (at 78.74 55.88) (layer F.SilkS) (tstamp 61816212)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 14 (at 78.74 63.5) (layer F.SilkS) (tstamp 61816211)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 24 (at 78.74 76.2) (layer F.SilkS) (tstamp 61816210)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 10 (at 78.74 58.42) (layer F.SilkS) (tstamp 6181620F)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 4 (at 78.74 50.8) (layer F.SilkS) (tstamp 6181620E)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 20 (at 78.74 71.12) (layer F.SilkS) (tstamp 6181620D)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 12 (at 78.74 60.96) (layer F.SilkS) (tstamp 6181620C)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 2 (at 78.74 48.26) (layer F.SilkS) (tstamp 6181620B)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 18 (at 78.74 68.58) (layer F.SilkS) (tstamp 6181620A)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 23 (at 71.12 76.2) (layer F.SilkS) (tstamp 6181613B)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 21 (at 71.12 73.66) (layer F.SilkS) (tstamp 61816139)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 19 (at 71.12 71.12) (layer F.SilkS) (tstamp 61816137)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 17 (at 71.12 68.58) (layer F.SilkS) (tstamp 61816135)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 15 (at 71.12 66.04) (layer F.SilkS) (tstamp 61816133)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 13 (at 71.12 63.5) (layer F.SilkS) (tstamp 61816131)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 11 (at 71.12 60.96) (layer F.SilkS) (tstamp 6181610D)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 9 (at 71.12 58.42) (layer F.SilkS) (tstamp 6181610B)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 7 (at 71.12 55.88) (layer F.SilkS) (tstamp 61816109)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 5 (at 71.12 53.34) (layer F.SilkS) (tstamp 61816107)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 3 (at 71.12 50.8) (layer F.SilkS) (tstamp 61816105)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_text 1 (at 71.12 48.26) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (gr_line (start 67.31 80.01) (end 67.31 44.45) (layer Edge.Cuts) (width 0.05) (tstamp 61816102))
  (gr_line (start 82.55 80.01) (end 67.31 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.55 44.45) (end 82.55 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 67.31 44.45) (end 82.55 44.45) (layer Edge.Cuts) (width 0.05))

  (segment (start 77.724 49.276) (end 81.28 45.72) (width 0.18) (layer F.Cu) (net 28) (tstamp 61816022) (status 20))
  (segment (start 75.675 59.6) (end 77.724 57.551) (width 0.18) (layer F.Cu) (net 28) (tstamp 61816025) (status 10))
  (segment (start 77.724 57.551) (end 77.724 49.276) (width 0.18) (layer F.Cu) (net 28) (tstamp 6181603D))
  (segment (start 78.486 57.544) (end 78.486 51.054) (width 0.18) (layer F.Cu) (net 27) (tstamp 6181601A))
  (segment (start 78.486 51.054) (end 81.28 48.26) (width 0.18) (layer F.Cu) (net 27) (tstamp 6181601B) (status 20))
  (segment (start 75.725 60.305) (end 78.486 57.544) (width 0.18) (layer F.Cu) (net 27) (tstamp 61816024) (status 10))
  (segment (start 79.248 52.832) (end 81.28 50.8) (width 0.18) (layer F.Cu) (net 26) (tstamp 61816013) (status 20))
  (segment (start 75.725 60.655) (end 75.997 60.655) (width 0.18) (layer F.Cu) (net 26) (tstamp 61816019) (status 10))
  (segment (start 79.248 57.404) (end 79.248 52.832) (width 0.18) (layer F.Cu) (net 26) (tstamp 61816026))
  (segment (start 75.997 60.655) (end 79.248 57.404) (width 0.18) (layer F.Cu) (net 26) (tstamp 61816039))
  (segment (start 80.01 54.61) (end 81.28 53.34) (width 0.18) (layer F.Cu) (net 25) (tstamp 6181601C) (status 20))
  (segment (start 75.725 61.005) (end 76.409 61.005) (width 0.18) (layer F.Cu) (net 25) (tstamp 61816030) (status 10))
  (segment (start 80.01 57.404) (end 80.01 54.61) (width 0.18) (layer F.Cu) (net 25) (tstamp 6181603A))
  (segment (start 76.409 61.005) (end 80.01 57.404) (width 0.18) (layer F.Cu) (net 25) (tstamp 6181603B))
  (segment (start 81.28 56.896) (end 81.28 55.88) (width 0.18) (layer F.Cu) (net 24) (tstamp 6181602C) (status 20))
  (segment (start 76.821 61.355) (end 81.28 56.896) (width 0.18) (layer F.Cu) (net 24) (tstamp 61816037))
  (segment (start 75.725 61.355) (end 76.821 61.355) (width 0.18) (layer F.Cu) (net 24) (tstamp 61816038) (status 10))
  (segment (start 75.725 61.705) (end 77.995 61.705) (width 0.18) (layer F.Cu) (net 23) (tstamp 6181601F) (status 10))
  (segment (start 77.995 61.705) (end 81.28 58.42) (width 0.18) (layer F.Cu) (net 23) (tstamp 61816020) (status 20))
  (segment (start 75.725 62.055) (end 80.185 62.055) (width 0.18) (layer F.Cu) (net 22) (tstamp 61816017) (status 10))
  (segment (start 80.185 62.055) (end 81.28 60.96) (width 0.18) (layer F.Cu) (net 22) (tstamp 61816021) (status 20))
  (segment (start 80.185 62.405) (end 81.28 63.5) (width 0.18) (layer F.Cu) (net 21) (tstamp 6181601D) (status 20))
  (segment (start 75.725 62.405) (end 80.185 62.405) (width 0.18) (layer F.Cu) (net 21) (tstamp 6181602F) (status 10))
  (segment (start 77.995 62.755) (end 81.28 66.04) (width 0.18) (layer F.Cu) (net 20) (tstamp 61816015) (status 20))
  (segment (start 75.725 62.755) (end 77.995 62.755) (width 0.18) (layer F.Cu) (net 20) (tstamp 61816034) (status 10))
  (segment (start 81.28 67.564) (end 81.28 68.58) (width 0.18) (layer F.Cu) (net 19) (tstamp 61816023) (status 20))
  (segment (start 76.821 63.105) (end 81.28 67.564) (width 0.18) (layer F.Cu) (net 19) (tstamp 61816036))
  (segment (start 75.725 63.105) (end 76.821 63.105) (width 0.18) (layer F.Cu) (net 19) (tstamp 6181603E) (status 10))
  (segment (start 80.01 69.85) (end 81.28 71.12) (width 0.18) (layer F.Cu) (net 18) (tstamp 61816027) (status 20))
  (segment (start 76.409 63.455) (end 80.01 67.056) (width 0.18) (layer F.Cu) (net 18) (tstamp 6181602A))
  (segment (start 80.01 67.056) (end 80.01 69.85) (width 0.18) (layer F.Cu) (net 18) (tstamp 61816033))
  (segment (start 75.725 63.455) (end 76.409 63.455) (width 0.18) (layer F.Cu) (net 18) (tstamp 61816035) (status 10))
  (segment (start 79.248 66.992398) (end 79.248 71.628) (width 0.18) (layer F.Cu) (net 17) (tstamp 61816028))
  (segment (start 79.248 71.628) (end 81.28 73.66) (width 0.18) (layer F.Cu) (net 17) (tstamp 61816029) (status 20))
  (segment (start 76.060602 63.805) (end 79.248 66.992398) (width 0.18) (layer F.Cu) (net 17) (tstamp 6181602D))
  (segment (start 75.725 63.805) (end 76.060602 63.805) (width 0.18) (layer F.Cu) (net 17) (tstamp 6181603C) (status 10))
  (segment (start 78.486 73.406) (end 81.28 76.2) (width 0.18) (layer F.Cu) (net 16) (tstamp 61816014) (status 20))
  (segment (start 75.725 64.155) (end 78.486 66.916) (width 0.18) (layer F.Cu) (net 16) (tstamp 61816016) (status 10))
  (segment (start 78.486 66.916) (end 78.486 73.406) (width 0.18) (layer F.Cu) (net 16) (tstamp 61816018))
  (segment (start 77.724 66.909) (end 77.724 75.184) (width 0.18) (layer F.Cu) (net 15) (tstamp 6181602E))
  (segment (start 77.724 75.184) (end 81.28 78.74) (width 0.18) (layer F.Cu) (net 15) (tstamp 61816031) (status 20))
  (segment (start 75.675 64.86) (end 77.724 66.909) (width 0.18) (layer F.Cu) (net 15) (tstamp 6181603F) (status 10))
  (segment (start 72.136 66.909) (end 72.136 75.184) (width 0.18) (layer F.Cu) (net 1))
  (segment (start 74.185 64.86) (end 72.136 66.909) (width 0.18) (layer F.Cu) (net 1) (status 10))
  (segment (start 72.136 75.184) (end 68.58 78.74) (width 0.18) (layer F.Cu) (net 1) (status 20))
  (segment (start 74.135 64.155) (end 71.374 66.916) (width 0.18) (layer F.Cu) (net 2) (status 10))
  (segment (start 71.374 73.406) (end 68.58 76.2) (width 0.18) (layer F.Cu) (net 2) (status 20))
  (segment (start 71.374 66.916) (end 71.374 73.406) (width 0.18) (layer F.Cu) (net 2))
  (segment (start 73.863 63.805) (end 70.612 67.056) (width 0.18) (layer F.Cu) (net 3))
  (segment (start 70.612 71.628) (end 68.58 73.66) (width 0.18) (layer F.Cu) (net 3) (status 20))
  (segment (start 70.612 67.056) (end 70.612 71.628) (width 0.18) (layer F.Cu) (net 3))
  (segment (start 74.135 63.805) (end 73.863 63.805) (width 0.18) (layer F.Cu) (net 3) (status 10))
  (segment (start 73.451 63.455) (end 69.85 67.056) (width 0.18) (layer F.Cu) (net 4))
  (segment (start 69.85 67.056) (end 69.85 69.85) (width 0.18) (layer F.Cu) (net 4))
  (segment (start 74.135 63.455) (end 73.451 63.455) (width 0.18) (layer F.Cu) (net 4) (status 10))
  (segment (start 69.85 69.85) (end 68.58 71.12) (width 0.18) (layer F.Cu) (net 4) (status 20))
  (segment (start 74.135 63.105) (end 73.039 63.105) (width 0.18) (layer F.Cu) (net 5) (status 10))
  (segment (start 73.039 63.105) (end 68.58 67.564) (width 0.18) (layer F.Cu) (net 5))
  (segment (start 68.58 67.564) (end 68.58 68.58) (width 0.18) (layer F.Cu) (net 5) (status 20))
  (segment (start 71.865 62.755) (end 68.58 66.04) (width 0.18) (layer F.Cu) (net 6) (status 20))
  (segment (start 74.135 62.755) (end 71.865 62.755) (width 0.18) (layer F.Cu) (net 6) (status 10))
  (segment (start 69.675 62.405) (end 68.58 63.5) (width 0.18) (layer F.Cu) (net 7) (status 20))
  (segment (start 74.135 62.405) (end 69.675 62.405) (width 0.18) (layer F.Cu) (net 7) (status 10))
  (segment (start 69.675 62.055) (end 68.58 60.96) (width 0.18) (layer F.Cu) (net 8) (status 20))
  (segment (start 74.135 62.055) (end 69.675 62.055) (width 0.18) (layer F.Cu) (net 8) (status 10))
  (segment (start 71.865 61.705) (end 68.58 58.42) (width 0.18) (layer F.Cu) (net 9) (status 20))
  (segment (start 74.135 61.705) (end 71.865 61.705) (width 0.18) (layer F.Cu) (net 9) (status 10))
  (segment (start 68.58 56.896) (end 68.58 55.88) (width 0.18) (layer F.Cu) (net 10) (status 20))
  (segment (start 73.039 61.355) (end 68.58 56.896) (width 0.18) (layer F.Cu) (net 10))
  (segment (start 74.135 61.355) (end 73.039 61.355) (width 0.18) (layer F.Cu) (net 10) (status 10))
  (segment (start 69.85 54.61) (end 68.58 53.34) (width 0.18) (layer F.Cu) (net 11) (status 20))
  (segment (start 69.85 57.404) (end 69.85 54.61) (width 0.18) (layer F.Cu) (net 11))
  (segment (start 73.451 61.005) (end 69.85 57.404) (width 0.18) (layer F.Cu) (net 11))
  (segment (start 74.135 61.005) (end 73.451 61.005) (width 0.18) (layer F.Cu) (net 11) (status 10))
  (segment (start 70.612 52.832) (end 68.58 50.8) (width 0.18) (layer F.Cu) (net 12) (status 20))
  (segment (start 70.612 57.467602) (end 70.612 52.832) (width 0.18) (layer F.Cu) (net 12))
  (segment (start 73.799398 60.655) (end 70.612 57.467602) (width 0.18) (layer F.Cu) (net 12))
  (segment (start 74.135 60.655) (end 73.799398 60.655) (width 0.18) (layer F.Cu) (net 12) (status 10))
  (segment (start 71.374 51.054) (end 68.58 48.26) (width 0.18) (layer F.Cu) (net 13) (status 20))
  (segment (start 71.374 57.544) (end 71.374 51.054) (width 0.18) (layer F.Cu) (net 13))
  (segment (start 74.135 60.305) (end 71.374 57.544) (width 0.18) (layer F.Cu) (net 13) (status 10))
  (segment (start 72.136 49.276) (end 68.58 45.72) (width 0.18) (layer F.Cu) (net 14) (status 20))
  (segment (start 72.136 57.551) (end 72.136 49.276) (width 0.18) (layer F.Cu) (net 14))
  (segment (start 74.185 59.6) (end 72.136 57.551) (width 0.18) (layer F.Cu) (net 14) (status 10))

)
