(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~90~ubuntu20.04.1)

  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 4)
    (zones 0)
    (modules 26)
    (nets 1)
  )

  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )

  (module lilygo_micro32:T-Micro32 (layer F.Cu) (tedit 61131E02) (tstamp 612AC4AA)
    (at 158.801 42.723)
    (fp_text reference REF** (at 2 -4.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value T-Micro32 (at 6.5 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3 5.5) (end 3 12.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 5.5) (end 3 5.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 12.5) (end 10 5.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 3 12.5) (end 10 12.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 -1.5) (end 13 -2) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 -1.5) (end 13 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start 8 -1.5) (end 12 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 -1.5) (end 10 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 8 -3.5) (end 4 -1.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 2 -1.5) (end 6 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -1.5) (end 4 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -2.5) (end 2 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 13 15.5) (end 13 15) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 15.5) (end 13 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 15.5) (end 2 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 15) (end 0 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 13 -3.5) (end 13 -1) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -3.5) (end 13 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -1) (end 0 -3.5) (layer F.SilkS) (width 0.15))
    (pad 1 smd rect (at 0 0) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 2) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0 3) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 4) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0 5) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 6) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 7) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0 8) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0 9) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 10) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0 11) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0 12) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0 13) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 0 14) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 3 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 4 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 5 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 6 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 7 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 8 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 9 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 10 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 13 14) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 13 13) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 13 12) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 13 11) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 13 10) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 13 9) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 13 8) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 13 7) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 13 6) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 13 5) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 13 4) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 13 3) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 13 2) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 13 1) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 38 smd rect (at 13 0) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
  )

  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C) (tstamp 612AC3AC)
    (at 146.228 100 90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference REF** (at 0 -2.45 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TSOP-6_1.65x3.05mm_P0.95mm (at 0 2.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.76 1.77) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.77) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.76 -1.78) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.76 -1.78) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.825 -1.525) (end 0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 1.525) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.1) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 -1.525) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.1) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -1.6) (end -1.5 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 1.6) (end 0.8 1.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 6 smd rect (at 1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.16 0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.16 0 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.16 -0.95 90) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module tube_mounts:5.5od_0.2thickness_no_pins (layer F.Cu) (tedit 612A700F) (tstamp 612AC32B)
    (at 146.99 100)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 5.5od_0.2thickness_no_pins (at 0 -0.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_poly (pts (xy 0.879 2.27) (xy 0.769 2.27) (xy 0.769 -2.23) (xy 0.889 -2.23)) (layer Dwgs.User) (width 0.01))
    (fp_circle (center 0 0) (end 2.9 0) (layer F.Mask) (width 0.8))
    (fp_circle (center 0 0) (end 2.9 0) (layer F.Cu) (width 0.7))
    (pad "" thru_hole oval (at 0.889 0) (size 0.6 5.05) (drill oval 0.35 4.8) (layers *.Cu *.Mask))
  )

  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C) (tstamp 612AC36C)
    (at 164.516 100)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference REF** (at 0 -2.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TSOP-6_1.65x3.05mm_P0.95mm (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.8 1.6) (end 0.8 1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.8 -1.6) (end -1.5 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.825 -1.1) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 -1.525) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.1) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 1.525) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 -1.525) (end 0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -1.76 -1.78) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.76 -1.78) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.77) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.77) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 1 smd rect (at -1.16 -0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.16 0) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.16 0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.16 0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.16 0) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.16 -0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm_ThermalVias (layer F.Cu) (tedit 5A671B3A) (tstamp 6128544B)
    (at 92.38 90.475)
    (descr "HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad")
    (tags "TSSOP HTSSOP 0.65 thermal pad")
    (attr smd)
    (fp_text reference REF** (at 0 -5.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm_ThermalVias (at 0 5.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -2.325 -4.75) (end -3.4 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.325 5.0258) (end 2.325 5.0258) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.325 -4.975) (end 2.325 -4.975) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.325 5.0258) (end -2.325 4.7008) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.325 5.0258) (end 2.325 4.7008) (layer F.SilkS) (width 0.15))
    (fp_line (start 2.325 -4.975) (end 2.325 -4.65) (layer F.SilkS) (width 0.15))
    (fp_line (start -2.325 -4.975) (end -2.325 -4.75) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.65 5.15) (end 3.65 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -5.15) (end 3.65 -5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.65 -5.15) (end 3.65 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.65 -5.15) (end -3.65 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.2 -3.85) (end -1.2 -4.85) (layer F.Fab) (width 0.15))
    (fp_line (start -2.2 4.85) (end -2.2 -3.85) (layer F.Fab) (width 0.15))
    (fp_line (start 2.2 4.9008) (end -2.2 4.9008) (layer F.Fab) (width 0.15))
    (fp_line (start 2.2 -4.85) (end 2.2 4.85) (layer F.Fab) (width 0.15))
    (fp_line (start -1.2 -4.85) (end 2.2 -4.85) (layer F.Fab) (width 0.15))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.15)))
    )
    (pad 29 smd rect (at 0 0) (size 3.4 9.7) (layers B.Cu))
    (pad "" smd rect (at -0.6 1.78) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at 0.6 1.78) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at -0.6 0) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at 0.6 0) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at 0.6 -1.78) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at -0.6 -1.78) (size 0.9 1.4) (layers F.Paste))
    (pad "" smd rect (at 0 0) (size 2.4 6.17) (layers F.Mask))
    (pad 29 thru_hole circle (at -1.3 4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at -1.3 2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at -1.3 0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at -1.3 -0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 -0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 -0.89) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at -1.3 -2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 -2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 -2.67) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 1.3 -4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at 0 -4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 thru_hole circle (at -1.3 -4.45) (size 0.6 0.6) (drill 0.3) (layers *.Cu))
    (pad 29 smd rect (at 0 0) (size 3.4 9.7) (layers F.Cu))
    (pad 28 smd rect (at 2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128489E)
    (at 119.853598 108.577625 70)
    (fp_text reference REF** (at 2.032 -1.397 70) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 70) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 70) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 70) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 70) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 70) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 61284886)
    (at 115.722559 114.850661 50)
    (fp_text reference REF** (at 2.032 -1.397 50) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 50) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 50) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 50) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 50) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 50) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128486E)
    (at 109.695148 119.332488 30)
    (fp_text reference REF** (at 2.032 -1.397 30) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 30) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 30) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 30) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 30) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 30) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 61284826)
    (at 88.105148 118.062488 330)
    (fp_text reference REF** (at 2.032 -1.397 150) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 150) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 330) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 330) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 330) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 330) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128480E)
    (at 82.64476 112.904908 310)
    (fp_text reference REF** (at 2.032 -1.397 130) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 130) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 310) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 310) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 310) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 310) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 612847F6)
    (at 79.277671 106.190805 290)
    (fp_text reference REF** (at 2.032 -1.397 110) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 110) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 290) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 290) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 290) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 290) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 612847DE)
    (at 78.41 98.73 270)
    (fp_text reference REF** (at 2.032 -1.397 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 270) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 270) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 270) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 270) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 612854B1)
    (at 80.146402 91.422375 250)
    (fp_text reference REF** (at 2.032 -1.397 70) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 70) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 250) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 250) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 250) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 250) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 612847AE)
    (at 84.277441 85.149339 230)
    (fp_text reference REF** (at 2.032 -1.397 50) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 50) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 230) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 230) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 230) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 230) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 61284796)
    (at 90.304852 80.667512 210)
    (fp_text reference REF** (at 2.032 -1.397 30) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 30) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 210) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 210) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 210) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 210) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128477E)
    (at 97.501642 78.517467 190)
    (fp_text reference REF** (at 2.032 -1.397 10) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 10) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 190) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 190) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 190) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 190) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 61284766)
    (at 104.99977 78.958534 170)
    (fp_text reference REF** (at 2.032 -1.397 170) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 170) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 170) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 170) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 170) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 170) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128474E)
    (at 111.894852 81.937512 150)
    (fp_text reference REF** (at 2.032 -1.397 150) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 150) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 150) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 150) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 150) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 150) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 61284736)
    (at 117.35524 87.095092 130)
    (fp_text reference REF** (at 2.032 -1.397 130) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 130) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 130) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 130) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 130) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 130) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 6128471E)
    (at 120.722329 93.809195 110)
    (fp_text reference REF** (at 2.032 -1.397 110) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 110) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (pad 1 smd custom (at 0 0 110) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
    (pad 2 smd rect (at 1.35 0 110) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at 2.375 0 110) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 4 smd custom (at 3.6 0 110) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
  )

  (module sk6812:SK6812-SIDE-A (layer F.Cu) (tedit 6127EC07) (tstamp 612841C3)
    (at 121.59 101.27 90)
    (fp_text reference REF** (at 2.032 -1.397 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SK6812-SIDE-A (at 0 -0.5 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.7 1.4) (end -0.7 -0.6) (layer F.SilkS) (width 0.1))
    (fp_line (start 3.7 1.4) (end -0.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 0.7) (end 3.7 1.4) (layer F.SilkS) (width 0.1))
    (fp_line (start 4.3 -0.6) (end 4.3 0.7) (layer F.SilkS) (width 0.1))
    (fp_line (start -0.7 -0.6) (end 4.3 -0.6) (layer F.SilkS) (width 0.1))
    (pad 4 smd custom (at 3.6 0 90) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.05 -0.525) (xy -0.5 -0.525) (xy -0.5 0.675) (xy 0.05 0.675)) (width 0))
      ))
    (pad 3 smd rect (at 2.375 0 90) (size 0.45 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 2 smd rect (at 1.35 0 90) (size 0.7 1.2) (drill (offset 0 0.075)) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0))
    (pad 1 smd custom (at 0 0 90) (size 1 0.55) (layers F.Cu F.Paste F.Mask)
      (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.05 -0.525) (xy 0.5 -0.525) (xy 0.5 0.675) (xy -0.05 0.675)) (width 0))
      ))
  )

  (module Connector_USB:USB_Micro-B_Amphenol_10104110_Horizontal (layer F.Cu) (tedit 5E5842A1) (tstamp 612815B4)
    (at 100 120.32)
    (descr "USB Micro-B, horizontal, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10104110.pdf")
    (tags "USB Micro B horizontal")
    (attr smd)
    (fp_text reference REF** (at 0 -3.55) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value USB_Micro-B_Amphenol_10104110_Horizontal (at 0 5.35) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -3.86 4.16) (end -3.86 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.86 -1.66) (end 1.8 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.86 0.05) (end 3.86 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.86 -1.66) (end -1.8 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.86 0.05) (end -3.86 -1.66) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.3 -1.85) (end -0.9 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -0.9 -2.25) (end -1.7 -2.25) (layer F.Fab) (width 0.1))
    (fp_line (start -1.7 -2.25) (end -1.3 -1.85) (layer F.Fab) (width 0.1))
    (fp_line (start -3.75 4.05) (end -3.75 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 4.05) (end -3.75 4.05) (layer F.Fab) (width 0.1))
    (fp_line (start 3.75 -1.55) (end 3.75 4.05) (layer F.Fab) (width 0.1))
    (fp_line (start -3.75 -1.55) (end 3.75 -1.55) (layer F.Fab) (width 0.1))
    (fp_line (start -2.6 2.75) (end 2.6 2.75) (layer F.Fab) (width 0.1))
    (fp_line (start -3.86 4.16) (end 3.86 4.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.86 4.16) (end 3.86 2.55) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.66) (end -1.8 -2.25) (layer F.SilkS) (width 0.12))
    (fp_line (start -5.4 -2.75) (end -5.4 4.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.4 4.55) (end 5.4 4.55) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.4 4.55) (end 5.4 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.4 -2.75) (end -5.4 -2.75) (layer F.CrtYd) (width 0.05))
    (fp_text user "PCB edge" (at 0 2.75) (layer Dwgs.User)
      (effects (font (size 0.5 0.5) (thickness 0.08)))
    )
    (fp_text user %R (at 0 -0.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (pad 1 smd rect (at -1.3 -1.55) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.65 -1.55) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.55) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.55) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.55) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -3.75 1.3) (size 2.3 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 3.75 1.3) (size 2.3 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.15 1.3) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.15 1.3) (size 1.8 1.9) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10104110_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:SOP-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5F476169) (tstamp 6128556A)
    (at 91.745 109.525)
    (descr "SOP, 16 Pin (https://www.diodes.com/assets/Datasheets/PAM8403.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (attr smd)
    (fp_text reference REF** (at 0 -5.9) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOP-16_3.9x9.9mm_P1.27mm (at 0 5.9) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 5.06) (end 1.95 5.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 5.06) (end -1.95 5.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.06) (end 1.95 -5.06) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -5.06) (end -3.5 -5.06) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -4.95) (end 1.95 -4.95) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -4.95) (end 1.95 4.95) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 4.95) (end -1.95 4.95) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 4.95) (end -1.95 -3.975) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -3.975) (end -0.975 -4.95) (layer F.Fab) (width 0.1))
    (fp_line (start -3.75 -5.2) (end -3.75 5.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 5.2) (end 3.75 5.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 5.2) (end 3.75 -5.2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 -5.2) (end -3.75 -5.2) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (pad 16 smd roundrect (at 2.5 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at 2.5 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 2.5 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 2.5 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 2.5 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 2.5 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 2.5 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 2.5 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -2.5 4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -2.5 3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -2.5 1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -2.5 0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -2.5 -0.635) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -2.5 -1.905) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.5 -3.175) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.5 -4.445) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOP-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module lilygo_micro32:T-Micro32 (layer F.Cu) (tedit 61131E02) (tstamp 61273CE3)
    (at 104.445 93.015)
    (fp_text reference REF** (at 2 -4.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value T-Micro32 (at 6.5 3) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 -1) (end 0 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -3.5) (end 13 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 13 -3.5) (end 13 -1) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 15) (end 0 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 15.5) (end 2 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 11 15.5) (end 13 15.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 13 15.5) (end 13 15) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -2.5) (end 2 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 0 -1.5) (end 4 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 2 -1.5) (end 6 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 8 -3.5) (end 4 -1.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 6 -1.5) (end 10 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 8 -1.5) (end 12 -3.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 -1.5) (end 13 -3) (layer F.SilkS) (width 0.15))
    (fp_line (start 12 -1.5) (end 13 -2) (layer F.SilkS) (width 0.15))
    (fp_line (start 3 12.5) (end 10 12.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 12.5) (end 10 5.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 10 5.5) (end 3 5.5) (layer F.SilkS) (width 0.15))
    (fp_line (start 3 5.5) (end 3 12.5) (layer F.SilkS) (width 0.15))
    (pad 38 smd rect (at 13 0) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 13 1) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 13 2) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 13 3) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 13 4) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 13 5) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 13 6) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 13 7) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 13 8) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 13 9) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 13 10) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 13 11) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 13 12) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 13 13) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 13 14) (size 2.1 0.7) (drill (offset 0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 10 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 9 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 8 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 7 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 6 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 5 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 4 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 3 15.5) (size 0.7 2.1) (drill (offset 0 0.3)) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 0 14) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0 13) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0 12) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0 11) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 10) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 0 9) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 0 8) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 0 7) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 0 6) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0 5) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 4) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0 3) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 2) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 0 0) (size 2.1 0.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask))
  )

  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1) (tstamp 61136B49)
    (at 47.295 73.965)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference REF** (at 0 -3.4) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SOIC-8_3.9x4.9mm_P1.27mm (at 0 3.4) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 0 2.56) (end 1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 2.56) (end -1.95 2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end 1.95 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0 -2.56) (end -3.45 -2.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.975 -2.45) (end 1.95 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 -2.45) (end 1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start 1.95 2.45) (end -1.95 2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 2.45) (end -1.95 -1.475) (layer F.Fab) (width 0.1))
    (fp_line (start -1.95 -1.475) (end -0.975 -2.45) (layer F.Fab) (width 0.1))
    (fp_line (start -3.7 -2.7) (end -3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.7 2.7) (end 3.7 2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 2.7) (end 3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.7 -2.7) (end -3.7 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.98 0.98) (thickness 0.15)))
    )
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_SO:TSOP-6_1.65x3.05mm_P0.95mm (layer F.Cu) (tedit 5A02F25C) (tstamp 6127CAA0)
    (at 100 100)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference REF** (at 0 -2.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value TSOP-6_1.65x3.05mm_P0.95mm (at 0 2.5) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 1.76 1.77) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.76 1.77) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.76 -1.78) (end -1.76 1.77) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.76 -1.78) (end 1.76 -1.78) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0.825 -1.525) (end 0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 1.525) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.1) (end -0.825 1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.825 -1.525) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start -0.825 -1.1) (end -0.425 -1.525) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -1.6) (end -1.5 -1.6) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.8 1.6) (end 0.8 1.6) (layer F.SilkS) (width 0.12))
    (fp_text user %R (at 0 0 90) (layer F.Fab)
      (effects (font (size 0.5 0.5) (thickness 0.075)))
    )
    (pad 6 smd rect (at 1.16 -0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.16 0) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.16 0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.16 0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.16 0) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.16 -0.95) (size 0.7 0.51) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_circle (center 150.8 49.2) (end 156.8 49.2) (layer Dwgs.User) (width 0.05))
  (gr_circle (center 150 50) (end 174.5 50) (layer Dwgs.User) (width 0.05))
  (gr_circle (center 150 50) (end 172.5 50) (layer Dwgs.User) (width 0.05))
  (gr_circle (center 161.748 100) (end 162.738 100) (layer Dwgs.User) (width 0.15))
  (gr_circle (center 163.5 100) (end 166.4 100) (layer Dwgs.User) (width 0.15))
  (gr_line (start 98.77 98.095) (end 101.27 98.095) (layer Dwgs.User) (width 0.15))
  (gr_circle (center 100 100) (end 100 76.5) (layer Dwgs.User) (width 0.15) (tstamp 61273FCC))
  (gr_circle (center 100 100) (end 101.25 100) (layer F.SilkS) (width 0.05))
  (gr_circle (center 100 100) (end 102.45 100) (layer F.SilkS) (width 0.12) (tstamp 61273B50))
  (gr_circle (center 100 100) (end 102.25 100) (layer F.SilkS) (width 0.12))
  (gr_circle (center 100 100) (end 117 100) (layer Edge.Cuts) (width 0.05))

  (segment (start 145.278 99.426) (end 145.212 99.492) (width 0.25) (layer F.Cu) (net 0))
  (via (at 145.212 99.492) (size 0.8) (drill 0.4) (layers F.Cu B.Cu) (net 0))
  (segment (start 145.278 98.84) (end 145.278 99.426) (width 0.25) (layer F.Cu) (net 0))
  (segment (start 145.212 99.492) (end 143.561 97.841) (width 0.25) (layer B.Cu) (net 0))

)
