(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 0)
    (zones 0)
    (modules 20)
    (nets 124)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(U1-Pad48)")
  (net 2 "Net-(U1-Pad47)")
  (net 3 "Net-(U1-Pad46)")
  (net 4 "Net-(U1-Pad45)")
  (net 5 "Net-(U1-Pad44)")
  (net 6 "Net-(U1-Pad43)")
  (net 7 "Net-(U1-Pad42)")
  (net 8 "Net-(U1-Pad41)")
  (net 9 "Net-(U1-Pad40)")
  (net 10 "Net-(U1-Pad39)")
  (net 11 "Net-(U1-Pad38)")
  (net 12 "Net-(U1-Pad37)")
  (net 13 "Net-(U1-Pad36)")
  (net 14 "Net-(U1-Pad35)")
  (net 15 "Net-(U1-Pad34)")
  (net 16 "Net-(U1-Pad33)")
  (net 17 "Net-(U1-Pad32)")
  (net 18 "Net-(U1-Pad31)")
  (net 19 "Net-(U1-Pad30)")
  (net 20 "Net-(U1-Pad29)")
  (net 21 "Net-(U1-Pad28)")
  (net 22 "Net-(U1-Pad27)")
  (net 23 "Net-(U1-Pad26)")
  (net 24 "Net-(U1-Pad25)")
  (net 25 "Net-(U1-Pad24)")
  (net 26 "Net-(U1-Pad23)")
  (net 27 "Net-(U1-Pad22)")
  (net 28 "Net-(U1-Pad21)")
  (net 29 "Net-(U1-Pad20)")
  (net 30 "Net-(U1-Pad19)")
  (net 31 "Net-(U1-Pad18)")
  (net 32 "Net-(U1-Pad17)")
  (net 33 "Net-(U1-Pad16)")
  (net 34 "Net-(U1-Pad15)")
  (net 35 "Net-(U1-Pad14)")
  (net 36 "Net-(U1-Pad13)")
  (net 37 "Net-(U1-Pad12)")
  (net 38 "Net-(U1-Pad11)")
  (net 39 "Net-(U1-Pad10)")
  (net 40 "Net-(U1-Pad9)")
  (net 41 "Net-(U1-Pad8)")
  (net 42 "Net-(U1-Pad7)")
  (net 43 "Net-(U1-Pad6)")
  (net 44 "Net-(U1-Pad5)")
  (net 45 "Net-(U1-Pad4)")
  (net 46 "Net-(U1-Pad3)")
  (net 47 "Net-(U1-Pad2)")
  (net 48 "Net-(U1-Pad1)")
  (net 49 GND)
  (net 50 MOT_RST)
  (net 51 MOT_EN0)
  (net 52 "Net-(R1-Pad2)")
  (net 53 MOT_REF1)
  (net 54 "Net-(M1-Pad3)")
  (net 55 "Net-(R5-Pad1)")
  (net 56 "Net-(M1-Pad4)")
  (net 57 +5V)
  (net 58 "Net-(M1-Pad1)")
  (net 59 "Net-(R7-Pad1)")
  (net 60 "Net-(M1-Pad2)")
  (net 61 MOT_STCK0)
  (net 62 MOT_DIR0)
  (net 63 MOT_EN1)
  (net 64 "Net-(R2-Pad2)")
  (net 65 "Net-(M2-Pad3)")
  (net 66 "Net-(R6-Pad1)")
  (net 67 "Net-(M2-Pad4)")
  (net 68 "Net-(M2-Pad1)")
  (net 69 "Net-(R8-Pad1)")
  (net 70 "Net-(M2-Pad2)")
  (net 71 MOT_STCK1)
  (net 72 MOT_DIR1)
  (net 73 "Net-(C1-Pad2)")
  (net 74 "Net-(C2-Pad2)")
  (net 75 I2C_SDA)
  (net 76 I2C_CLK)
  (net 77 "Net-(J2-Pad40)")
  (net 78 "Net-(J2-Pad39)")
  (net 79 "Net-(J2-Pad38)")
  (net 80 "Net-(J2-Pad37)")
  (net 81 "Net-(J2-Pad36)")
  (net 82 "Net-(J2-Pad35)")
  (net 83 "Net-(J2-Pad34)")
  (net 84 "Net-(J2-Pad33)")
  (net 85 "Net-(J2-Pad32)")
  (net 86 "Net-(J2-Pad31)")
  (net 87 "Net-(J2-Pad30)")
  (net 88 "Net-(J2-Pad29)")
  (net 89 "Net-(J2-Pad28)")
  (net 90 "Net-(J2-Pad27)")
  (net 91 "Net-(J2-Pad26)")
  (net 92 "Net-(J2-Pad25)")
  (net 93 "Net-(J2-Pad24)")
  (net 94 "Net-(J2-Pad23)")
  (net 95 "Net-(J2-Pad22)")
  (net 96 "Net-(J2-Pad21)")
  (net 97 "Net-(J2-Pad20)")
  (net 98 "Net-(J2-Pad19)")
  (net 99 "Net-(J2-Pad18)")
  (net 100 "Net-(J2-Pad17)")
  (net 101 "Net-(J2-Pad16)")
  (net 102 "Net-(J2-Pad15)")
  (net 103 "Net-(J2-Pad14)")
  (net 104 "Net-(J2-Pad13)")
  (net 105 "Net-(J2-Pad12)")
  (net 106 "Net-(J2-Pad11)")
  (net 107 "Net-(J2-Pad10)")
  (net 108 "Net-(J2-Pad9)")
  (net 109 "Net-(J2-Pad8)")
  (net 110 "Net-(J2-Pad7)")
  (net 111 "Net-(J2-Pad6)")
  (net 112 "Net-(J2-Pad5)")
  (net 113 "Net-(J2-Pad4)")
  (net 114 "Net-(J2-Pad3)")
  (net 115 "Net-(J2-Pad2)")
  (net 116 "Net-(J2-Pad1)")
  (net 117 SDC)
  (net 118 SDO)
  (net 119 +3v3)
  (net 120 ADDR3)
  (net 121 ADDR2)
  (net 122 ADDR1)
  (net 123 ADDR0)

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3v3)
    (add_net +5V)
    (add_net ADDR0)
    (add_net ADDR1)
    (add_net ADDR2)
    (add_net ADDR3)
    (add_net GND)
    (add_net I2C_CLK)
    (add_net I2C_SDA)
    (add_net MOT_DIR0)
    (add_net MOT_DIR1)
    (add_net MOT_EN0)
    (add_net MOT_EN1)
    (add_net MOT_REF1)
    (add_net MOT_RST)
    (add_net MOT_STCK0)
    (add_net MOT_STCK1)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad39)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M2-Pad1)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M2-Pad3)")
    (add_net "Net-(M2-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net SDC)
    (add_net SDO)
  )

  (module Button_Switch_THT:SW_DIP_SPSTx06_Slide_9.78x17.42mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1405) (tstamp 6063DB97)
    (at 52.832 -7.493)
    (descr "6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x17.42mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (path /60BCB5AC)
    (fp_text reference SW1 (at 3.81 -3.42) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value SW_DIP_x04 (at 3.81 16.12) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (fp_text user %R (at 7.27 6.35 90) (layer F.Fab)
      (effects (font (size 0.8 0.8) (thickness 0.12)))
    )
    (fp_line (start -0.08 -2.36) (end 8.7 -2.36) (layer F.Fab) (width 0.1))
    (fp_line (start 8.7 -2.36) (end 8.7 15.06) (layer F.Fab) (width 0.1))
    (fp_line (start 8.7 15.06) (end -1.08 15.06) (layer F.Fab) (width 0.1))
    (fp_line (start -1.08 15.06) (end -1.08 -1.36) (layer F.Fab) (width 0.1))
    (fp_line (start -1.08 -1.36) (end -0.08 -2.36) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.635) (end 1.78 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.635) (end 5.84 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 0.635) (end 5.84 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 -0.635) (end 1.78 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.535) (end 3.133333 -0.535) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.435) (end 3.133333 -0.435) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.335) (end 3.133333 -0.335) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.235) (end 3.133333 -0.235) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.135) (end 3.133333 -0.135) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 -0.035) (end 3.133333 -0.035) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.065) (end 3.133333 0.065) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.165) (end 3.133333 0.165) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.265) (end 3.133333 0.265) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.365) (end 3.133333 0.365) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.465) (end 3.133333 0.465) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 0.565) (end 3.133333 0.565) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 -0.635) (end 3.133333 0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 1.905) (end 1.78 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 3.175) (end 5.84 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 3.175) (end 5.84 1.905) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 1.905) (end 1.78 1.905) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.005) (end 3.133333 2.005) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.105) (end 3.133333 2.105) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.205) (end 3.133333 2.205) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.305) (end 3.133333 2.305) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.405) (end 3.133333 2.405) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.505) (end 3.133333 2.505) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.605) (end 3.133333 2.605) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.705) (end 3.133333 2.705) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.805) (end 3.133333 2.805) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 2.905) (end 3.133333 2.905) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 3.005) (end 3.133333 3.005) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 3.105) (end 3.133333 3.105) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 1.905) (end 3.133333 3.175) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.445) (end 1.78 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.715) (end 5.84 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 5.715) (end 5.84 4.445) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 4.445) (end 1.78 4.445) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.545) (end 3.133333 4.545) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.645) (end 3.133333 4.645) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.745) (end 3.133333 4.745) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.845) (end 3.133333 4.845) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 4.945) (end 3.133333 4.945) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.045) (end 3.133333 5.045) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.145) (end 3.133333 5.145) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.245) (end 3.133333 5.245) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.345) (end 3.133333 5.345) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.445) (end 3.133333 5.445) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.545) (end 3.133333 5.545) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 5.645) (end 3.133333 5.645) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 4.445) (end 3.133333 5.715) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 6.985) (end 1.78 8.255) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 8.255) (end 5.84 8.255) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 8.255) (end 5.84 6.985) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 6.985) (end 1.78 6.985) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.085) (end 3.133333 7.085) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.185) (end 3.133333 7.185) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.285) (end 3.133333 7.285) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.385) (end 3.133333 7.385) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.485) (end 3.133333 7.485) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.585) (end 3.133333 7.585) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.685) (end 3.133333 7.685) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.785) (end 3.133333 7.785) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.885) (end 3.133333 7.885) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 7.985) (end 3.133333 7.985) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 8.085) (end 3.133333 8.085) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 8.185) (end 3.133333 8.185) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 6.985) (end 3.133333 8.255) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 9.525) (end 1.78 10.795) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.795) (end 5.84 10.795) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 10.795) (end 5.84 9.525) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 9.525) (end 1.78 9.525) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 9.625) (end 3.133333 9.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 9.725) (end 3.133333 9.725) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 9.825) (end 3.133333 9.825) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 9.925) (end 3.133333 9.925) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.025) (end 3.133333 10.025) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.125) (end 3.133333 10.125) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.225) (end 3.133333 10.225) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.325) (end 3.133333 10.325) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.425) (end 3.133333 10.425) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.525) (end 3.133333 10.525) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.625) (end 3.133333 10.625) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 10.725) (end 3.133333 10.725) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 9.525) (end 3.133333 10.795) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.065) (end 1.78 13.335) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 13.335) (end 5.84 13.335) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 13.335) (end 5.84 12.065) (layer F.Fab) (width 0.1))
    (fp_line (start 5.84 12.065) (end 1.78 12.065) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.165) (end 3.133333 12.165) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.265) (end 3.133333 12.265) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.365) (end 3.133333 12.365) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.465) (end 3.133333 12.465) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.565) (end 3.133333 12.565) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.665) (end 3.133333 12.665) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.765) (end 3.133333 12.765) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.865) (end 3.133333 12.865) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 12.965) (end 3.133333 12.965) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 13.065) (end 3.133333 13.065) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 13.165) (end 3.133333 13.165) (layer F.Fab) (width 0.1))
    (fp_line (start 1.78 13.265) (end 3.133333 13.265) (layer F.Fab) (width 0.1))
    (fp_line (start 3.133333 12.065) (end 3.133333 13.335) (layer F.Fab) (width 0.1))
    (fp_line (start -1.14 -2.42) (end 8.76 -2.42) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.14 15.12) (end 8.76 15.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.14 -2.42) (end -1.14 15.12) (layer F.SilkS) (width 0.12))
    (fp_line (start 8.76 -2.42) (end 8.76 15.12) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.38 -2.66) (end 0.004 -2.66) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.38 -2.66) (end -1.38 -1.277) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.635) (end 1.78 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.635) (end 5.84 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 0.635) (end 5.84 -0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 -0.635) (end 1.78 -0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.515) (end 3.133333 -0.515) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.395) (end 3.133333 -0.395) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.275) (end 3.133333 -0.275) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.155) (end 3.133333 -0.155) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 -0.035) (end 3.133333 -0.035) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.085) (end 3.133333 0.085) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.205) (end 3.133333 0.205) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.325) (end 3.133333 0.325) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.445) (end 3.133333 0.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 0.565) (end 3.133333 0.565) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 -0.635) (end 3.133333 0.635) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 1.905) (end 1.78 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 3.175) (end 5.84 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 3.175) (end 5.84 1.905) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 1.905) (end 1.78 1.905) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.025) (end 3.133333 2.025) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.145) (end 3.133333 2.145) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.265) (end 3.133333 2.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.385) (end 3.133333 2.385) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.505) (end 3.133333 2.505) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.625) (end 3.133333 2.625) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.745) (end 3.133333 2.745) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.865) (end 3.133333 2.865) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 2.985) (end 3.133333 2.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 3.105) (end 3.133333 3.105) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 1.905) (end 3.133333 3.175) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.445) (end 1.78 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.715) (end 5.84 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 5.715) (end 5.84 4.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 4.445) (end 1.78 4.445) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.565) (end 3.133333 4.565) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.685) (end 3.133333 4.685) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.805) (end 3.133333 4.805) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 4.925) (end 3.133333 4.925) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.045) (end 3.133333 5.045) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.165) (end 3.133333 5.165) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.285) (end 3.133333 5.285) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.405) (end 3.133333 5.405) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.525) (end 3.133333 5.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 5.645) (end 3.133333 5.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 4.445) (end 3.133333 5.715) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 6.985) (end 1.78 8.255) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 8.255) (end 5.84 8.255) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 8.255) (end 5.84 6.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 6.985) (end 1.78 6.985) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.105) (end 3.133333 7.105) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.225) (end 3.133333 7.225) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.345) (end 3.133333 7.345) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.465) (end 3.133333 7.465) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.585) (end 3.133333 7.585) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.705) (end 3.133333 7.705) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.825) (end 3.133333 7.825) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 7.945) (end 3.133333 7.945) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 8.065) (end 3.133333 8.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 8.185) (end 3.133333 8.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 6.985) (end 3.133333 8.255) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 9.525) (end 1.78 10.795) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.795) (end 5.84 10.795) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 10.795) (end 5.84 9.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 9.525) (end 1.78 9.525) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 9.645) (end 3.133333 9.645) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 9.765) (end 3.133333 9.765) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 9.885) (end 3.133333 9.885) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.005) (end 3.133333 10.005) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.125) (end 3.133333 10.125) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.245) (end 3.133333 10.245) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.365) (end 3.133333 10.365) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.485) (end 3.133333 10.485) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.605) (end 3.133333 10.605) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 10.725) (end 3.133333 10.725) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 9.525) (end 3.133333 10.795) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.065) (end 1.78 13.335) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 13.335) (end 5.84 13.335) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 13.335) (end 5.84 12.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 5.84 12.065) (end 1.78 12.065) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.185) (end 3.133333 12.185) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.305) (end 3.133333 12.305) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.425) (end 3.133333 12.425) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.545) (end 3.133333 12.545) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.665) (end 3.133333 12.665) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.785) (end 3.133333 12.785) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 12.905) (end 3.133333 12.905) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 13.025) (end 3.133333 13.025) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 13.145) (end 3.133333 13.145) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.78 13.265) (end 3.133333 13.265) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.133333 12.065) (end 3.133333 13.335) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.35 -2.7) (end -1.35 15.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.35 15.4) (end 8.95 15.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.95 15.4) (end 8.95 -2.7) (layer F.CrtYd) (width 0.05))
    (fp_line (start 8.95 -2.7) (end -1.35 -2.7) (layer F.CrtYd) (width 0.05))
    (pad 12 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 11 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 10 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 ADDR3))
    (pad 9 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 ADDR2))
    (pad 8 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 ADDR1))
    (pad 7 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 ADDR0))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx06_Slide_9.78x17.42mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DAB6)
    (at -21.315 -12.952)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BB2E3C)
    (attr smd)
    (fp_text reference R8 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330mE (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DAA5)
    (at -25.325 -12.952)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BB47EF)
    (attr smd)
    (fp_text reference R7 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330mE (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA94)
    (at -17.305 -15.462)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BB01AD)
    (attr smd)
    (fp_text reference R6 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330mE (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA83)
    (at -21.315 -15.462)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BB457F)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 330mE (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA72)
    (at -25.325 -15.462)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BF2DDC)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47K (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA61)
    (at -13.915 -19.852)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60C05757)
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47K (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA50)
    (at -9.905 -22.362)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60BF36D6)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47K (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063DA3F)
    (at -13.915 -22.362)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (path /60C0575D)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 47K (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4125) (end -0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4125) (end 0.8 -0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4125) (end 0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4125) (end -0.8 0.4125) (layer F.Fab) (width 0.1))
    (fp_line (start -0.237258 -0.5225) (end 0.237258 -0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.237258 0.5225) (end 0.237258 0.5225) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6063DA2E)
    (at -33.02 -54.61)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /60BD39C6)
    (fp_text reference J6 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 SDC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 SDO))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 +3v3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6063EACB)
    (at -3.81 66.04 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /60BBB19E)
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 I2C_SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 I2C_CLK))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6063D9FE)
    (at -4.295 -66.04 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /60BBA98A)
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 I2C_SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 I2C_CLK))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6063E955)
    (at 66.04 -4.064)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /60BBA03E)
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.309 -1.129 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 I2C_SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 I2C_CLK))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB) (tstamp 6063D9CE)
    (at -40.955 -33.542)
    (descr "Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x20 2.54mm double row")
    (path /60BC7AC8)
    (fp_text reference J2 (at 5.655 -2.27) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Raspberry_Pi_2_3 (at 5.655 50.53) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5.31 24.13 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 4.675 -1.27) (end 6.58 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 -1.27) (end 6.58 49.53) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 49.53) (end 4.04 49.53) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 49.53) (end 4.04 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start 4.04 -0.635) (end 4.675 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end 4.04 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 -0.32) (end -0.32 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 0.32) (end 4.04 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 -0.32) (end 12.58 -0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 -0.32) (end 12.58 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 0.32) (end 12.58 0.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end 4.04 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.22) (end -0.32 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 2.86) (end 4.04 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 2.22) (end 12.58 2.22) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 2.22) (end 12.58 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 2.86) (end 12.58 2.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end 4.04 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 4.76) (end -0.32 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 5.4) (end 4.04 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 4.76) (end 12.58 4.76) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 4.76) (end 12.58 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 5.4) (end 12.58 5.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end 4.04 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.3) (end -0.32 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 7.94) (end 4.04 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 7.3) (end 12.58 7.3) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 7.3) (end 12.58 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 7.94) (end 12.58 7.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end 4.04 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 9.84) (end -0.32 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 10.48) (end 4.04 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 9.84) (end 12.58 9.84) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 9.84) (end 12.58 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 10.48) (end 12.58 10.48) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 12.38) (end 4.04 12.38) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 12.38) (end -0.32 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 13.02) (end 4.04 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 12.38) (end 12.58 12.38) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 12.38) (end 12.58 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 13.02) (end 12.58 13.02) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 14.92) (end 4.04 14.92) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 14.92) (end -0.32 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 15.56) (end 4.04 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 14.92) (end 12.58 14.92) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 14.92) (end 12.58 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 15.56) (end 12.58 15.56) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 17.46) (end 4.04 17.46) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 17.46) (end -0.32 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 18.1) (end 4.04 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 17.46) (end 12.58 17.46) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 17.46) (end 12.58 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 18.1) (end 12.58 18.1) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20) (end 4.04 20) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20) (end -0.32 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 20.64) (end 4.04 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 20) (end 12.58 20) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 20) (end 12.58 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 20.64) (end 12.58 20.64) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 22.54) (end 4.04 22.54) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 22.54) (end -0.32 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 23.18) (end 4.04 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 22.54) (end 12.58 22.54) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 22.54) (end 12.58 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 23.18) (end 12.58 23.18) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.08) (end 4.04 25.08) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.08) (end -0.32 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 25.72) (end 4.04 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 25.08) (end 12.58 25.08) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 25.08) (end 12.58 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 25.72) (end 12.58 25.72) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 27.62) (end 4.04 27.62) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 27.62) (end -0.32 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 28.26) (end 4.04 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 27.62) (end 12.58 27.62) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 27.62) (end 12.58 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 28.26) (end 12.58 28.26) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.16) (end 4.04 30.16) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.16) (end -0.32 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 30.8) (end 4.04 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 30.16) (end 12.58 30.16) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 30.16) (end 12.58 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 30.8) (end 12.58 30.8) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 32.7) (end 4.04 32.7) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 32.7) (end -0.32 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 33.34) (end 4.04 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 32.7) (end 12.58 32.7) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 32.7) (end 12.58 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 33.34) (end 12.58 33.34) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.24) (end 4.04 35.24) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.24) (end -0.32 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 35.88) (end 4.04 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 35.24) (end 12.58 35.24) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 35.24) (end 12.58 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 35.88) (end 12.58 35.88) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 37.78) (end 4.04 37.78) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 37.78) (end -0.32 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 38.42) (end 4.04 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 37.78) (end 12.58 37.78) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 37.78) (end 12.58 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 38.42) (end 12.58 38.42) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.32) (end 4.04 40.32) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.32) (end -0.32 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 40.96) (end 4.04 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 40.32) (end 12.58 40.32) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 40.32) (end 12.58 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 40.96) (end 12.58 40.96) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 42.86) (end 4.04 42.86) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 42.86) (end -0.32 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 43.5) (end 4.04 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 42.86) (end 12.58 42.86) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 42.86) (end 12.58 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 43.5) (end 12.58 43.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 45.4) (end 4.04 45.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 45.4) (end -0.32 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 46.04) (end 4.04 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 45.4) (end 12.58 45.4) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 45.4) (end 12.58 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 46.04) (end 12.58 46.04) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 47.94) (end 4.04 47.94) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 47.94) (end -0.32 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start -0.32 48.58) (end 4.04 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 47.94) (end 12.58 47.94) (layer F.Fab) (width 0.1))
    (fp_line (start 12.58 47.94) (end 12.58 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start 6.58 48.58) (end 12.58 48.58) (layer F.Fab) (width 0.1))
    (fp_line (start 3.98 -1.33) (end 3.98 49.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 49.59) (end 6.64 49.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 49.59) (end 6.64 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 -1.33) (end 3.98 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 -0.38) (end 12.64 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 -0.38) (end 12.64 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 0.38) (end 6.64 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 -0.32) (end 12.64 -0.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 -0.2) (end 12.64 -0.2) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 -0.08) (end 12.64 -0.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 0.04) (end 12.64 0.04) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 0.16) (end 12.64 0.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 0.28) (end 12.64 0.28) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 -0.38) (end 3.98 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 0.38) (end 3.98 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 -0.38) (end 1.497071 -0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.11 0.38) (end 1.497071 0.38) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 1.27) (end 6.64 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 2.16) (end 12.64 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 2.16) (end 12.64 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 2.92) (end 6.64 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 2.16) (end 3.98 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 2.92) (end 3.98 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.16) (end 1.497071 2.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 2.92) (end 1.497071 2.92) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 3.81) (end 6.64 3.81) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 4.7) (end 12.64 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 4.7) (end 12.64 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 5.46) (end 6.64 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 4.7) (end 3.98 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 5.46) (end 3.98 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 4.7) (end 1.497071 4.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 5.46) (end 1.497071 5.46) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 6.35) (end 6.64 6.35) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 7.24) (end 12.64 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 7.24) (end 12.64 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 8) (end 6.64 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 7.24) (end 3.98 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 8) (end 3.98 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 7.24) (end 1.497071 7.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 8) (end 1.497071 8) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 8.89) (end 6.64 8.89) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 9.78) (end 12.64 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 9.78) (end 12.64 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 10.54) (end 6.64 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 9.78) (end 3.98 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 10.54) (end 3.98 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 9.78) (end 1.497071 9.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 10.54) (end 1.497071 10.54) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 11.43) (end 6.64 11.43) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 12.32) (end 12.64 12.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 12.32) (end 12.64 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 13.08) (end 6.64 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 12.32) (end 3.98 12.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 13.08) (end 3.98 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 12.32) (end 1.497071 12.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 13.08) (end 1.497071 13.08) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 13.97) (end 6.64 13.97) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 14.86) (end 12.64 14.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 14.86) (end 12.64 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 15.62) (end 6.64 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 14.86) (end 3.98 14.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 15.62) (end 3.98 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 14.86) (end 1.497071 14.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 15.62) (end 1.497071 15.62) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 16.51) (end 6.64 16.51) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 17.4) (end 12.64 17.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 17.4) (end 12.64 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 18.16) (end 6.64 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 17.4) (end 3.98 17.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 18.16) (end 3.98 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 17.4) (end 1.497071 17.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 18.16) (end 1.497071 18.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 19.05) (end 6.64 19.05) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 19.94) (end 12.64 19.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 19.94) (end 12.64 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 20.7) (end 6.64 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 19.94) (end 3.98 19.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 20.7) (end 3.98 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 19.94) (end 1.497071 19.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 20.7) (end 1.497071 20.7) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 21.59) (end 6.64 21.59) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 22.48) (end 12.64 22.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 22.48) (end 12.64 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 23.24) (end 6.64 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 22.48) (end 3.98 22.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 23.24) (end 3.98 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 22.48) (end 1.497071 22.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 23.24) (end 1.497071 23.24) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 24.13) (end 6.64 24.13) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 25.02) (end 12.64 25.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 25.02) (end 12.64 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 25.78) (end 6.64 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 25.02) (end 3.98 25.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 25.78) (end 3.98 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 25.02) (end 1.497071 25.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 25.78) (end 1.497071 25.78) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 26.67) (end 6.64 26.67) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 27.56) (end 12.64 27.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 27.56) (end 12.64 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 28.32) (end 6.64 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 27.56) (end 3.98 27.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 28.32) (end 3.98 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 27.56) (end 1.497071 27.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 28.32) (end 1.497071 28.32) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 29.21) (end 6.64 29.21) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 30.1) (end 12.64 30.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 30.1) (end 12.64 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 30.86) (end 6.64 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 30.1) (end 3.98 30.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 30.86) (end 3.98 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 30.1) (end 1.497071 30.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 30.86) (end 1.497071 30.86) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 31.75) (end 6.64 31.75) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 32.64) (end 12.64 32.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 32.64) (end 12.64 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 33.4) (end 6.64 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 32.64) (end 3.98 32.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 33.4) (end 3.98 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 32.64) (end 1.497071 32.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 33.4) (end 1.497071 33.4) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 34.29) (end 6.64 34.29) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 35.18) (end 12.64 35.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 35.18) (end 12.64 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 35.94) (end 6.64 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 35.18) (end 3.98 35.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 35.94) (end 3.98 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 35.18) (end 1.497071 35.18) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 35.94) (end 1.497071 35.94) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 36.83) (end 6.64 36.83) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 37.72) (end 12.64 37.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 37.72) (end 12.64 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 38.48) (end 6.64 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 37.72) (end 3.98 37.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 38.48) (end 3.98 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 37.72) (end 1.497071 37.72) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 38.48) (end 1.497071 38.48) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 39.37) (end 6.64 39.37) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 40.26) (end 12.64 40.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 40.26) (end 12.64 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 41.02) (end 6.64 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 40.26) (end 3.98 40.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 41.02) (end 3.98 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 40.26) (end 1.497071 40.26) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 41.02) (end 1.497071 41.02) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 41.91) (end 6.64 41.91) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 42.8) (end 12.64 42.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 42.8) (end 12.64 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 43.56) (end 6.64 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 42.8) (end 3.98 42.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 43.56) (end 3.98 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 42.8) (end 1.497071 42.8) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 43.56) (end 1.497071 43.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 44.45) (end 6.64 44.45) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 45.34) (end 12.64 45.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 45.34) (end 12.64 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 46.1) (end 6.64 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 45.34) (end 3.98 45.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 46.1) (end 3.98 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 45.34) (end 1.497071 45.34) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 46.1) (end 1.497071 46.1) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.98 46.99) (end 6.64 46.99) (layer F.SilkS) (width 0.12))
    (fp_line (start 6.64 47.88) (end 12.64 47.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 47.88) (end 12.64 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 12.64 48.64) (end 6.64 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 47.88) (end 3.98 47.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.582929 48.64) (end 3.98 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 47.88) (end 1.497071 47.88) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.042929 48.64) (end 1.497071 48.64) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 0) (end -1.27 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.27 -1.27) (end 0 -1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 50.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 50.05) (end 13.1 50.05) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.1 50.05) (end 13.1 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 13.1 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J2-Pad40)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J2-Pad39)"))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J2-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J2-Pad37)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J2-Pad36)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J2-Pad35)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J2-Pad34)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J2-Pad33)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J2-Pad32)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(J2-Pad31)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(J2-Pad30)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(J2-Pad29)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(J2-Pad28)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(J2-Pad27)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J2-Pad26)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J2-Pad25)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J2-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(J2-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(J2-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(J2-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(J2-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(J2-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(J2-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(J2-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC) (tstamp 6063D875)
    (at -64.77 -3.937)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (path /60BB9569)
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 3.81 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 -1.27) (end 1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start 1.27 8.89) (end -1.27 8.89) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 8.89) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27) (layer F.Fab) (width 0.1))
    (fp_line (start -1.33 8.95) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end -1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.33 1.27) (end 1.33 8.95) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.8 -1.8) (end -1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.8 9.4) (end 1.8 9.4) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 9.4) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 I2C_SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 I2C_CLK))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063D85D)
    (at 9.335 -34.612)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /60BFA833)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22nF (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(C2-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE) (tstamp 6063D84C)
    (at -41.275 18.288)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (path /60C05763)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value 22nF (at 0 1.43) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 0.4 0.4) (thickness 0.06)))
    )
    (fp_line (start -0.8 0.4) (end -0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.8 -0.4) (end 0.8 -0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 -0.4) (end 0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start 0.8 0.4) (end -0.8 0.4) (layer F.Fab) (width 0.1))
    (fp_line (start -0.14058 -0.51) (end 0.14058 -0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.14058 0.51) (end 0.14058 0.51) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.48 0.73) (end -1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.48 -0.73) (end 1.48 -0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 -0.73) (end 1.48 0.73) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.48 0.73) (end -1.48 0.73) (layer F.CrtYd) (width 0.05))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5DC5F6A8) (tstamp 6063D2A1)
    (at 1.72 8.07)
    (descr "VQFN, 16 Pin (https://www.st.com/resource/en/datasheet/stspin220.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (path /60BA7446)
    (attr smd)
    (fp_text reference U3 (at 0 -2.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STSPIN220 (at 0 2.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 5.08 1.143) (layer F.Fab)
      (effects (font (size 0.75 0.75) (thickness 0.11)))
    )
    (fp_line (start 1.135 -1.61) (end 1.61 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -1.61) (end 1.61 -1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.135 1.61) (end -1.61 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 1.61) (end -1.61 1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.135 1.61) (end 1.61 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.61) (end 1.61 1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.135 -1.61) (end -1.61 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.12 -2.12) (end -2.12 2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.12 2.12) (end 2.12 2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.12 2.12) (end 2.12 -2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.12 -2.12) (end -2.12 -2.12) (layer F.CrtYd) (width 0.05))
    (pad "" smd roundrect (at 0.45 0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.45 -0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.45 0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.45 -0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 17 smd rect (at 0 0) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 49 GND))
    (pad 16 smd roundrect (at -0.75 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 15 smd roundrect (at -0.25 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 14 smd roundrect (at 0.25 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 MOT_RST))
    (pad 13 smd roundrect (at 0.75 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 MOT_EN1))
    (pad 12 smd roundrect (at 1.4875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(R2-Pad2)"))
    (pad 11 smd roundrect (at 1.4875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 MOT_REF1))
    (pad 10 smd roundrect (at 1.4875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(M2-Pad3)"))
    (pad 9 smd roundrect (at 1.4875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(R6-Pad1)"))
    (pad 8 smd roundrect (at 0.75 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(M2-Pad4)"))
    (pad 7 smd roundrect (at 0.25 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 6 smd roundrect (at -0.25 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 +5V))
    (pad 5 smd roundrect (at -0.75 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(M2-Pad1)"))
    (pad 4 smd roundrect (at -1.4875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(R8-Pad1)"))
    (pad 3 smd roundrect (at -1.4875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(M2-Pad2)"))
    (pad 2 smd roundrect (at -1.4875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 MOT_STCK1))
    (pad 1 smd roundrect (at -1.4875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 MOT_DIR1))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5DC5F6A8) (tstamp 6063D078)
    (at 2.54 -25.4)
    (descr "VQFN, 16 Pin (https://www.st.com/resource/en/datasheet/stspin220.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (path /60BA5CA4)
    (attr smd)
    (fp_text reference U2 (at 0 -2.82) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STSPIN220 (at 0 2.82) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at -6.096 -4.699) (layer F.Fab)
      (effects (font (size 0.75 0.75) (thickness 0.11)))
    )
    (fp_line (start 1.135 -1.61) (end 1.61 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 -1.61) (end 1.61 -1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.135 1.61) (end -1.61 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.61 1.61) (end -1.61 1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.135 1.61) (end 1.61 1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 1.61 1.61) (end 1.61 1.135) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.135 -1.61) (end -1.61 -1.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer F.Fab) (width 0.1))
    (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -2.12 -2.12) (end -2.12 2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start -2.12 2.12) (end 2.12 2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.12 2.12) (end 2.12 -2.12) (layer F.CrtYd) (width 0.05))
    (fp_line (start 2.12 -2.12) (end -2.12 -2.12) (layer F.CrtYd) (width 0.05))
    (pad "" smd roundrect (at 0.45 0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.45 -0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.45 0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.45 -0.45) (size 0.73 0.73) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 17 smd rect (at 0 0) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 49 GND))
    (pad 16 smd roundrect (at -0.75 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 15 smd roundrect (at -0.25 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 14 smd roundrect (at 0.25 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 MOT_RST))
    (pad 13 smd roundrect (at 0.75 -1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 MOT_EN0))
    (pad 12 smd roundrect (at 1.4875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(R1-Pad2)"))
    (pad 11 smd roundrect (at 1.4875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 MOT_REF1))
    (pad 10 smd roundrect (at 1.4875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(M1-Pad3)"))
    (pad 9 smd roundrect (at 1.4875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(R5-Pad1)"))
    (pad 8 smd roundrect (at 0.75 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(M1-Pad4)"))
    (pad 7 smd roundrect (at 0.25 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 6 smd roundrect (at -0.25 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 +5V))
    (pad 5 smd roundrect (at -0.75 1.4875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(M1-Pad1)"))
    (pad 4 smd roundrect (at -1.4875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R7-Pad1)"))
    (pad 3 smd roundrect (at -1.4875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(M1-Pad2)"))
    (pad 2 smd roundrect (at -1.4875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 MOT_STCK0))
    (pad 1 smd roundrect (at -1.4875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 MOT_DIR0))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Package_QFP:LQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5D9F72AF) (tstamp 6063D04E)
    (at 31.75 -45.72)
    (descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (path /60BADD13)
    (attr smd)
    (fp_text reference U1 (at 0 -5.85) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value STM32F103C8Tx (at 0 5.85) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 3.16 3.61) (end 3.61 3.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.61 3.61) (end 3.61 3.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.16 3.61) (end -3.61 3.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.61 3.61) (end -3.61 3.16) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.16 -3.61) (end 3.61 -3.61) (layer F.SilkS) (width 0.12))
    (fp_line (start 3.61 -3.61) (end 3.61 -3.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.16 -3.61) (end -3.61 -3.61) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.61 -3.61) (end -3.61 -3.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -3.61 -3.16) (end -4.9 -3.16) (layer F.SilkS) (width 0.12))
    (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer F.Fab) (width 0.1))
    (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0 -5.15) (end -3.15 -5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 -5.15) (end -3.15 -3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 -3.75) (end -3.75 -3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.75) (end -3.75 -3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 -3.15) (end -5.15 -3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 -3.15) (end -5.15 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 -5.15) (end 3.15 -5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 -5.15) (end 3.15 -3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 -3.75) (end 3.75 -3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 -3.75) (end 3.75 -3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 -3.15) (end 5.15 -3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.15 -3.15) (end 5.15 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 5.15) (end -3.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 5.15) (end -3.15 3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.15 3.75) (end -3.75 3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.75) (end -3.75 3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -3.75 3.15) (end -5.15 3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start -5.15 3.15) (end -5.15 0) (layer F.CrtYd) (width 0.05))
    (fp_line (start 0 5.15) (end 3.15 5.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 5.15) (end 3.15 3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.15 3.75) (end 3.75 3.75) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.75) (end 3.75 3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 3.75 3.15) (end 5.15 3.15) (layer F.CrtYd) (width 0.05))
    (fp_line (start 5.15 3.15) (end 5.15 0) (layer F.CrtYd) (width 0.05))
    (pad 48 smd roundrect (at -2.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U1-Pad48)"))
    (pad 47 smd roundrect (at -2.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(U1-Pad47)"))
    (pad 46 smd roundrect (at -1.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(U1-Pad46)"))
    (pad 45 smd roundrect (at -1.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(U1-Pad45)"))
    (pad 44 smd roundrect (at -0.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(U1-Pad44)"))
    (pad 43 smd roundrect (at -0.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(U1-Pad43)"))
    (pad 42 smd roundrect (at 0.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(U1-Pad42)"))
    (pad 41 smd roundrect (at 0.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(U1-Pad41)"))
    (pad 40 smd roundrect (at 1.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad40)"))
    (pad 39 smd roundrect (at 1.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad39)"))
    (pad 38 smd roundrect (at 2.25 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad38)"))
    (pad 37 smd roundrect (at 2.75 -4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(U1-Pad37)"))
    (pad 36 smd roundrect (at 4.1625 -2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(U1-Pad36)"))
    (pad 35 smd roundrect (at 4.1625 -2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(U1-Pad35)"))
    (pad 34 smd roundrect (at 4.1625 -1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(U1-Pad34)"))
    (pad 33 smd roundrect (at 4.1625 -1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(U1-Pad33)"))
    (pad 32 smd roundrect (at 4.1625 -0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(U1-Pad32)"))
    (pad 31 smd roundrect (at 4.1625 -0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(U1-Pad31)"))
    (pad 30 smd roundrect (at 4.1625 0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(U1-Pad30)"))
    (pad 29 smd roundrect (at 4.1625 0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(U1-Pad29)"))
    (pad 28 smd roundrect (at 4.1625 1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(U1-Pad28)"))
    (pad 27 smd roundrect (at 4.1625 1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(U1-Pad27)"))
    (pad 26 smd roundrect (at 4.1625 2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(U1-Pad26)"))
    (pad 25 smd roundrect (at 4.1625 2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(U1-Pad25)"))
    (pad 24 smd roundrect (at 2.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(U1-Pad24)"))
    (pad 23 smd roundrect (at 2.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad23)"))
    (pad 22 smd roundrect (at 1.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad22)"))
    (pad 21 smd roundrect (at 1.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(U1-Pad21)"))
    (pad 20 smd roundrect (at 0.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(U1-Pad20)"))
    (pad 19 smd roundrect (at 0.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(U1-Pad19)"))
    (pad 18 smd roundrect (at -0.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(U1-Pad18)"))
    (pad 17 smd roundrect (at -0.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(U1-Pad17)"))
    (pad 16 smd roundrect (at -1.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(U1-Pad16)"))
    (pad 15 smd roundrect (at -1.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(U1-Pad15)"))
    (pad 14 smd roundrect (at -2.25 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(U1-Pad14)"))
    (pad 13 smd roundrect (at -2.75 4.1625) (size 0.3 1.475) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(U1-Pad13)"))
    (pad 12 smd roundrect (at -4.1625 2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(U1-Pad12)"))
    (pad 11 smd roundrect (at -4.1625 2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(U1-Pad11)"))
    (pad 10 smd roundrect (at -4.1625 1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(U1-Pad10)"))
    (pad 9 smd roundrect (at -4.1625 1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(U1-Pad9)"))
    (pad 8 smd roundrect (at -4.1625 0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(U1-Pad8)"))
    (pad 7 smd roundrect (at -4.1625 0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at -4.1625 -0.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U1-Pad6)"))
    (pad 5 smd roundrect (at -4.1625 -0.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(U1-Pad5)"))
    (pad 4 smd roundrect (at -4.1625 -1.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(U1-Pad4)"))
    (pad 3 smd roundrect (at -4.1625 -1.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U1-Pad3)"))
    (pad 2 smd roundrect (at -4.1625 -2.25) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(U1-Pad2)"))
    (pad 1 smd roundrect (at -4.1625 -2.75) (size 1.475 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_circle (center -45 -45) (end -42.8 -45) (layer Edge.Cuts) (width 0.05) (tstamp 6063ED2C))
  (gr_circle (center 45 -45) (end 47.2 -45) (layer Edge.Cuts) (width 0.05) (tstamp 6063ED2C))
  (gr_circle (center 45 45) (end 47.2 45) (layer Edge.Cuts) (width 0.05) (tstamp 6063ED2A))
  (gr_circle (center -45 45) (end -42.8 45) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 0 0) (end 70 0) (layer Edge.Cuts) (width 0.05))

)
