(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")

  (general
    (thickness 1.6)
    (drawings 39)
    (tracks 19)
    (zones 0)
    (modules 12)
    (nets 6)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x014fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "OUTPUT"))
  )

  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(TP1-Pad1)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J2-Pad2)")

  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(TP1-Pad1)")
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2BBF)
    (at 142.19936 121.00052)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E3C25)
    (attr virtual)
    (fp_text reference H10 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2BB7)
    (at 171.1198 120.7262)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E396C)
    (attr virtual)
    (fp_text reference H9 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2D16)
    (at 171.10964 -24.85136)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E3763)
    (attr virtual)
    (fp_text reference H8 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2BA7)
    (at 170.7896 105.84688)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E2FC4)
    (attr virtual)
    (fp_text reference H7 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2B9F)
    (at 159.90824 -24.92248)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E3E0C)
    (attr virtual)
    (fp_text reference H6 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2B8F)
    (at 160.05048 -17.97304)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E4145)
    (attr virtual)
    (fp_text reference H4 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2B87)
    (at 171.25188 -17.8308)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E4322)
    (attr virtual)
    (fp_text reference H3 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2B7F)
    (at 128.41732 120.91416)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E45E4)
    (attr virtual)
    (fp_text reference H2 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765) (tstamp 619D2B77)
    (at 128.524 106.5276)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (path /619E483B)
    (attr virtual)
    (fp_text reference H1 (at 0 -3.2) (layer F.SilkS) hide
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value MountingHole (at 0 3.2) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0.3 0) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 0 0) (end 2.1 0) (layer Cmts.User) (width 0.15))
    (fp_circle (center 0 0) (end 2.35 0) (layer F.CrtYd) (width 0.05))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )

  (module MySymbols:bt_player (layer F.Cu) (tedit 619CCB48) (tstamp 619D2440)
    (at 154.184151 115.48892 180)
    (path /619DC5C9)
    (fp_text reference U1 (at 8.6 5.5) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value bt_player (at 8.464351 -7.42168) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user ANT (at -6.05 2.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user SPK (at -6.1 -2.45) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user BATT (at 8 -3.3) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_arc (start 0.05 0) (end 8.206739 -0.809999) (angle -54.93281825) (layer Dwgs.User) (width 0.12))
    (fp_arc (start -0.05 0) (end -4.049999 -7.183119) (angle -111.6079807) (layer Dwgs.User) (width 0.12))
    (fp_line (start 5.95 -0.81) (end 8.20674 -0.81) (layer Dwgs.User) (width 0.12))
    (fp_line (start 5.95 -1.75) (end 5.95 -0.81) (layer Dwgs.User) (width 0.12))
    (fp_line (start 4.05 -1.75) (end 4.05 -7.1755) (layer Dwgs.User) (width 0.12))
    (fp_line (start 5.95 -1.75) (end 4.05 -1.75) (layer Dwgs.User) (width 0.12))
    (fp_line (start -5.25 5.25) (end -4.05 5.25) (layer Dwgs.User) (width 0.12))
    (fp_line (start -5.25 6.35762) (end -5.25 5.25) (layer Dwgs.User) (width 0.12))
    (fp_line (start -4.05 5.25) (end -4.05 -7.18312) (layer Dwgs.User) (width 0.12))
    (pad 1 thru_hole circle (at -6.25 4.25 180) (size 1 1) (drill 0.3) (layers *.Cu *.Mask)
      (net 3 "Net-(TP1-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 -3.9 180) (size 1 1) (drill 0.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at -5.1 -5.1 180) (size 1 1) (drill 0.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 5 thru_hole circle (at 6.8 -1.75 180) (size 1 1) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 5.25 -3.75 180) (size 1 1) (drill 0.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
  )

  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738) (tstamp 619D2426)
    (at 165.1 -17.05356 90)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (path /619CCC7F)
    (fp_text reference J2 (at 0 -1.56 90) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02 (at 0.7112 4.21132 90) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0.5) (layer F.Fab)
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    )
    (fp_line (start -0.3175 -0.5) (end 0.635 -0.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.5) (end 0.635 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 1.5) (end -0.635 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 1.5) (end -0.635 -0.1825) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -0.1825) (end -0.3175 -0.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.695 1.56) (end -0.394493 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.394493 1.56) (end 0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0.685) (end -0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.695 0.685) (end 0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0.685) (end -0.608276 0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.608276 0.685) (end 0.695 0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0) (end -0.695 -0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 -0.685) (end 0 -0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1) (end -1.15 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2) (end 1.15 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.15 2) (end 1.15 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.15 -1) (end -1.15 -1) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 0 1 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical (layer F.Cu) (tedit 59FED738) (tstamp 619D240E)
    (at 142.84452 107.59516)
    (descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.00mm single row")
    (path /619CD972)
    (fp_text reference J1 (at 0 -1.56) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value Conn_01x02 (at 0 2.56) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user %R (at 0 0.5 90) (layer F.Fab)
      (effects (font (size 0.76 0.76) (thickness 0.114)))
    )
    (fp_line (start -0.3175 -0.5) (end 0.635 -0.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 -0.5) (end 0.635 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start 0.635 1.5) (end -0.635 1.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 1.5) (end -0.635 -0.1825) (layer F.Fab) (width 0.1))
    (fp_line (start -0.635 -0.1825) (end -0.3175 -0.5) (layer F.Fab) (width 0.1))
    (fp_line (start -0.695 1.56) (end -0.394493 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.394493 1.56) (end 0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0.685) (end -0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.695 0.685) (end 0.695 1.56) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0.685) (end -0.608276 0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start 0.608276 0.685) (end 0.695 0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 0) (end -0.695 -0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -0.695 -0.685) (end 0 -0.685) (layer F.SilkS) (width 0.12))
    (fp_line (start -1.15 -1) (end -1.15 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start -1.15 2) (end 1.15 2) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.15 2) (end 1.15 -1) (layer F.CrtYd) (width 0.05))
    (fp_line (start 1.15 -1) (end -1.15 -1) (layer F.CrtYd) (width 0.05))
    (pad 2 thru_hole oval (at 0 1) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_line (start 158.17088 -14.25092) (end 163.07308 -9.34872) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.974 -14.25092) (end 168.0718 -9.3472) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.974 -26.70556) (end 172.974 -14.25092) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.17088 -26.70556) (end 158.17088 -14.25092) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.0718 95.10268) (end 168.0718 -9.3472) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.07308 95.0976) (end 163.07308 -9.34872) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.17088 100) (end 163.07308 95.0976) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.974 100) (end 168.0718 95.10268) (layer Edge.Cuts) (width 0.05))
  (dimension 46.192447 (width 0.15) (layer Dwgs.User)
    (gr_text "46.192 mm" (at 149.885937 126.301212 -0.03150542931) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 126.79172 122.64644) (xy 126.79011 125.574932)))
    (feature2 (pts (xy 172.98416 122.67184) (xy 172.98255 125.600332)))
    (crossbar (pts (xy 172.982872 125.013912) (xy 126.790432 124.988512)))
    (arrow1a (pts (xy 126.790432 124.988512) (xy 127.917258 124.402711)))
    (arrow1b (pts (xy 126.790432 124.988512) (xy 127.916613 125.575552)))
    (arrow2a (pts (xy 172.982872 125.013912) (xy 171.856691 124.426872)))
    (arrow2b (pts (xy 172.982872 125.013912) (xy 171.856046 125.599713)))
  )
  (dimension 149.36724 (width 0.15) (layer Dwgs.User)
    (gr_text "149.367 mm" (at 177.821186 47.988384 89.99805136) (layer Dwgs.User)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (feature1 (pts (xy 172.97908 122.67184) (xy 177.105067 122.67198)))
    (feature2 (pts (xy 172.98416 -26.6954) (xy 177.110147 -26.69526)))
    (crossbar (pts (xy 176.523726 -26.69528) (xy 176.518646 122.67196)))
    (arrow1a (pts (xy 176.518646 122.67196) (xy 175.932264 121.545436)))
    (arrow1b (pts (xy 176.518646 122.67196) (xy 177.105105 121.545476)))
    (arrow2a (pts (xy 176.523726 -26.69528) (xy 175.937267 -25.568796)))
    (arrow2b (pts (xy 176.523726 -26.69528) (xy 177.110108 -25.568756)))
  )
  (gr_line (start 172.974 -26.70556) (end 158.17088 -26.70048) (layer Eco1.User) (width 0.15) (tstamp 619D2A2E))
  (gr_line (start 172.974 -16.25092) (end 172.974 -26.70556) (layer Eco1.User) (width 0.15))
  (gr_line (start 158.17088 -16.25092) (end 172.974 -16.25092) (layer Eco1.User) (width 0.15))
  (gr_line (start 158.17088 -26.70048) (end 158.17088 -16.25092) (layer Eco1.User) (width 0.15))
  (gr_line (start 158.17088 104.8258) (end 126.79172 104.8258) (layer Eco1.User) (width 0.15))
  (gr_line (start 158.17088 103.4288) (end 158.17088 104.8258) (layer Eco1.User) (width 0.15))
  (gr_line (start 172.974 103.4288) (end 158.17088 103.4288) (layer Eco1.User) (width 0.15))
  (gr_line (start 172.974 122.66676) (end 172.974 103.4288) (layer Eco1.User) (width 0.15))
  (gr_line (start 162.60572 122.66676) (end 172.974 122.66676) (layer Eco1.User) (width 0.15))
  (gr_line (start 162.60572 107.16768) (end 162.60572 122.66676) (layer Eco1.User) (width 0.15))
  (gr_line (start 145.62836 107.16768) (end 162.60572 107.16768) (layer Eco1.User) (width 0.15))
  (gr_line (start 145.62836 122.65152) (end 145.62836 107.16768) (layer Eco1.User) (width 0.15))
  (gr_line (start 126.79172 122.65152) (end 145.62836 122.65152) (layer Eco1.User) (width 0.15))
  (gr_line (start 126.79172 104.8258) (end 126.79172 122.65152) (layer Eco1.User) (width 0.15))
  (gr_line (start 172.974 122.66676) (end 158.242 122.66676) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172.974 100) (end 172.974 122.66676) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.17088 -26.70556) (end 172.974 -26.70556) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.17088 104.8258) (end 158.17088 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.79172 104.8258) (end 158.17088 104.8258) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.79172 122.65152) (end 126.79172 104.8258) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.1394 122.65152) (end 126.79172 122.65152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150.1394 117.23624) (end 150.1394 122.65152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.22932 117.23624) (end 150.1394 117.23624) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 148.22932 117.23624) (end 148.22932 116.30152) (layer Edge.Cuts) (width 0.05) (tstamp 619D28B3))
  (gr_line (start 148.22932 116.30152) (end 145.961627 116.296591) (layer Edge.Cuts) (width 0.05) (tstamp 619D28B1))
  (gr_arc (start 154.18308 115.4938) (end 159.435799 109.118401) (angle -135.062272) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.4358 110.236) (end 159.435799 109.118401) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.242 110.236) (end 159.4358 110.236) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.242 122.66676) (end 158.242 110.236) (layer Edge.Cuts) (width 0.05))

  (segment (start 144.1704 108.26496) (end 143.5006 107.59516) (width 0.6096) (layer F.Cu) (net 1))
  (segment (start 143.5006 107.59516) (end 142.84452 107.59516) (width 0.6096) (layer F.Cu) (net 1))
  (segment (start 144.92492 117.23892) (end 144.1704 116.4844) (width 0.6096) (layer F.Cu) (net 1))
  (segment (start 144.1704 116.4844) (end 144.1704 108.26496) (width 0.6096) (layer F.Cu) (net 1))
  (segment (start 147.384151 117.23892) (end 144.92492 117.23892) (width 0.6096) (layer F.Cu) (net 1))
  (segment (start 165.1 -17.05356) (end 165.1 -17.018) (width 0.25) (layer F.Cu) (net 2))
  (segment (start 164.592 -16.51) (end 164.592 -15.24) (width 0.6096) (layer F.Cu) (net 2))
  (segment (start 165.1 -17.018) (end 164.592 -16.51) (width 0.6096) (layer F.Cu) (net 2))
  (segment (start 164.592 117.348) (end 164.592 -15.24) (width 1.27) (layer F.Cu) (net 2))
  (segment (start 162.55108 119.38892) (end 164.592 117.348) (width 0.6096) (layer F.Cu) (net 2))
  (segment (start 160.284151 119.38892) (end 162.55108 119.38892) (width 0.6096) (layer F.Cu) (net 2))
  (segment (start 142.84452 116.87048) (end 145.21296 119.23892) (width 0.6096) (layer F.Cu) (net 4))
  (segment (start 145.21296 119.23892) (end 148.934151 119.23892) (width 0.6096) (layer F.Cu) (net 4))
  (segment (start 142.84452 108.59516) (end 142.84452 116.87048) (width 0.6096) (layer F.Cu) (net 4))
  (segment (start 166.1 -17.05356) (end 166.624 -16.52956) (width 0.6096) (layer F.Cu) (net 5))
  (segment (start 166.624 -16.52956) (end 166.624 -15.24) (width 0.6096) (layer F.Cu) (net 5))
  (segment (start 166.624 -15.24) (end 166.624 117.3226) (width 1.27) (layer F.Cu) (net 5))
  (segment (start 163.35768 120.58892) (end 159.284151 120.58892) (width 0.6096) (layer F.Cu) (net 5))
  (segment (start 166.624 117.3226) (end 163.35768 120.58892) (width 0.6096) (layer F.Cu) (net 5))

)
