# My-TTGO-Watch

A smartwatch based on ESP32 from LlyGo. Currently under development.

# Install

Clone this repository and open it with platformIO. Build and upload. On a terminal in vscode you can do it with
```bash
pio run -t upload
```

# how to make a screenshot

The firmware has an integrated webserver. Over this a screenshot can be triggered. The image has the format RGB565 and can be read with gimp. From bash it look like this
```bash
wget x.x.x.x/shot ; wget x.x.x.x/screen.565
```

# Interface

![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen1.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen2.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen3.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen4.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen5.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen6.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen7.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen8.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen9.png)
![screenshot](https://github.com/sharandac/My-TTGO-Watch/blob/master/images/screen10.png)
