(module 532610371 (layer F.Cu) (tedit 620AE163)
  (fp_text reference REF** (at 1.25 -3.02) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value CON_532610371 (at 1.25 -5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -3.453991 0) (end -4.977991 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start -4.977991 -0.635) (end -4.977991 0.635) (layer F.Fab) (width 0.1))
  (fp_line (start -4.977991 0.635) (end -3.453991 0) (layer F.Fab) (width 0.1))
  (fp_line (start -3.199991 -0.2) (end -3.199991 1.07996) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.199991 5) (end 5.699991 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.699991 5) (end 5.699991 4.720039) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.699991 -0.2) (end 3.22004 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.199991 5) (end 5.699991 5) (layer F.Fab) (width 0.1))
  (fp_line (start 5.699991 5) (end 5.699991 -0.2) (layer F.Fab) (width 0.1))
  (fp_line (start 5.699991 -0.2) (end -3.199991 -0.2) (layer F.Fab) (width 0.1))
  (fp_line (start -3.199991 -0.2) (end -3.199991 5) (layer F.Fab) (width 0.1))
  (fp_line (start -0.72004 -0.2) (end -3.199991 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.199991 4.720039) (end -3.199991 5) (layer F.SilkS) (width 0.12))
  (fp_line (start 5.699991 1.07996) (end 5.699991 -0.2) (layer F.SilkS) (width 0.12))
  (fp_line (start -4 -1) (end -4 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 5.5) (end 6.5 5.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.5 5.5) (end 6.5 -1) (layer F.CrtYd) (width 0.05))
  (fp_line (start 6.5 -1) (end -4 -1) (layer F.CrtYd) (width 0.05))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User)
    (effects (font (size 0.127 0.127) (thickness 0.002)))
  )
  (fp_text user 532610371 (at 1.25 -11.57) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user PICOBLADE_1.25_WIRE_TO_BOARD_WAFER_ASSY_SMT_-3_CKT (at 1.25 -9.03) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user NOTE (at -3.199991 9.960001) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user MAXIMUM_PACKAGE_HEIGHT:_3.4_MM (at -3.199991 12.500001) (layer Cmts.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 smd rect (at 0 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.25 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.5 0) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at -2.55 2.899999) (size 2.1 2.999999) (layers F.Cu F.Paste F.Mask))
  (pad "" smd rect (at 5.05 2.899999) (size 2.1 2.999999) (layers F.Cu F.Paste F.Mask))
  (model ${KIPRJMOD}/../lib/Molex.3dshapes/532610371.stp
    (offset (xyz 1.25 -4 1.9))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
)
