<!-- markdownlint-configure-file {
  "MD013": {
    "code_blocks": false,
    "tables": false
  },
  "MD033": false,
  "MD041": false
} -->

<div align="center">

# AWTRIX LIGHT

![GitHub all releases](https://img.shields.io/github/downloads/blueforcer/awtrix-light/total?style=flat-square)
![GitHub Sponsors](https://img.shields.io/github/sponsors/blueforcer?style=flat-square)
![Discord](https://img.shields.io/discord/546407049148366859?label=Discord&style=flat-square)
[![Compile](https://github.com/Blueforcer/awtrix-light/actions/workflows/main.yml/badge.svg?branch=main)](https://github.com/Blueforcer/awtrix-light/actions/workflows/main.yml)
    

![GIF-230324_161917](https://user-images.githubusercontent.com/31169771/227567565-3780ee83-1158-4371-9390-fd03a7873496.gif)
</div>

AWTRIX Light is an open‑source custom firmware for the [Ulanzi Smart Pixel clock TC001](https://www.ulanzi.com/products/ulanzi-pixel-smart-clock-2882) which lives on your smarthome.

It is ready to use straight out of the box, with time, date, temperature, and humidity pages pre-installed. You don't need to do anything other than turning it on to start using these features.    

However, for those with more advanced skills, the customization options available with customapps and mqtt commands allows you to take Awtrix Light to its full potential.
Just send all your customapps from your smarthome via MQTT and update it in realtime.
The powerful icon system bring your ideas to life and enjoy a hassle-free experience   

Join the thousands of satisfied awtrix users who have already chosen Awtrix 2 and Awtrix Light and experience the difference today! 

# Features
- Easy to setup
- Homeassistant discovery
- Onscreen menu where you can change your settings directly on the device
- Pre-installed Apps like time, date, temperature, humidity and battery
- Add customapps without recompiling straight from your Smarthome.
- Easy to use icon system
- Powerful MQTT commands
- RTTTL melody player
- Integrated filebrowser
- No cloud 
- No telemetry

# Getting Started

Starting is easy as 1-2-3
[with the documentation](https://blueforcer.github.io/awtrix-light/)


# Community  
Join the discord channel with over 1500 Users  
https://discord.gg/cyBCpdx  
