(module 3,5mm_straight_circular (layer F.Cu) (tedit 6027E55C)
  (fp_text reference REF** (at 0 -4) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value 3,5mm_straight_circular (at 0 3) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_circle (center 0 0) (end 8 0) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole oval (at 0 -2.5) (size 3.2 1.4) (drill oval 2.6 0.8) (layers *.Cu *.Mask)
    (die_length 1))
  (pad 2 thru_hole oval (at -2.5 0 90) (size 3.2 1.4) (drill oval 2.6 0.8) (layers *.Cu *.Mask)
    (die_length 1))
  (pad 3 thru_hole oval (at 2.5 0 90) (size 3.2 1.4) (drill oval 2.6 0.8) (layers *.Cu *.Mask)
    (die_length 1))
)
