(export (version D)
  (design
    (source /Users/willemoldemans/Documents/PROJECTEN/leo_3led_truck/manufacturing/CAD/ledTruck/ledTruck.sch)
    (date "2021 February 13, Saturday 19:21:43")
    (tool "Eeschema (5.1.9-0-10_14)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source ledTruck.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref CON1)
      (value SJ1-3523N)
      (footprint MySymbols:3,5mm_straight_circular)
      (datasheet https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
      (fields
        (field (name Category) "Connectors, Interconnects")
        (field (name DK_Datasheet_Link) https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
        (field (name DK_Detail_Page) /product-detail/en/cui-inc/SJ1-3523N/CP1-3523N-ND/738689)
        (field (name Description) "CONN JACK STEREO 3.5MM R/A")
        (field (name Digi-Key_PN) CP1-3523N-ND)
        (field (name Family) "Barrel - Audio Connectors")
        (field (name MPN) SJ1-3523N)
        (field (name Manufacturer) "CUI Inc.")
        (field (name Status) Active))
      (libsource (lib dk_Barrel-Audio-Connectors) (part SJ1-3523N) (description "CONN JACK STEREO 3.5MM R/A"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6021CA8A))
    (comp (ref CON2)
      (value SJ1-3523N)
      (footprint MySymbols:3,5mm_straight_circular)
      (datasheet https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
      (fields
        (field (name Category) "Connectors, Interconnects")
        (field (name DK_Datasheet_Link) https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
        (field (name DK_Detail_Page) /product-detail/en/cui-inc/SJ1-3523N/CP1-3523N-ND/738689)
        (field (name Description) "CONN JACK STEREO 3.5MM R/A")
        (field (name Digi-Key_PN) CP1-3523N-ND)
        (field (name Family) "Barrel - Audio Connectors")
        (field (name MPN) SJ1-3523N)
        (field (name Manufacturer) "CUI Inc.")
        (field (name Status) Active))
      (libsource (lib dk_Barrel-Audio-Connectors) (part SJ1-3523N) (description "CONN JACK STEREO 3.5MM R/A"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6021DB86))
    (comp (ref CON3)
      (value SJ1-3523N)
      (footprint MySymbols:3,5mm_straight_circular)
      (datasheet https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
      (fields
        (field (name Category) "Connectors, Interconnects")
        (field (name DK_Datasheet_Link) https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
        (field (name DK_Detail_Page) /product-detail/en/cui-inc/SJ1-3523N/CP1-3523N-ND/738689)
        (field (name Description) "CONN JACK STEREO 3.5MM R/A")
        (field (name Digi-Key_PN) CP1-3523N-ND)
        (field (name Family) "Barrel - Audio Connectors")
        (field (name MPN) SJ1-3523N)
        (field (name Manufacturer) "CUI Inc.")
        (field (name Status) Active))
      (libsource (lib dk_Barrel-Audio-Connectors) (part SJ1-3523N) (description "CONN JACK STEREO 3.5MM R/A"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6021F7DC))
    (comp (ref U2)
      (value MCP73832T-2ACI_OT)
      (footprint digikey-footprints:SOT-753)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
      (fields
        (field (name Category) "Integrated Circuits (ICs)")
        (field (name DK_Datasheet_Link) http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
        (field (name DK_Detail_Page) /product-detail/en/microchip-technology/MCP73832T-2ACI-OT/MCP73832T-2ACI-OTCT-ND/1979805)
        (field (name Description) "IC LI-ION/LI-POLY CTRLR SOT23-5")
        (field (name Digi-Key_PN) MCP73832T-2ACI/OTCT-ND)
        (field (name Family) "PMIC - Battery Chargers")
        (field (name MPN) MCP73832T-2ACI/OT)
        (field (name Manufacturer) "Microchip Technology")
        (field (name Status) Active))
      (libsource (lib dk_PMIC-Battery-Chargers) (part MCP73832T-2ACI_OT) (description "IC LI-ION/LI-POLY CTRLR SOT23-5"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60220E3E))
    (comp (ref J1)
      (value Conn_01x02_Male)
      (footprint Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60232097))
    (comp (ref J2)
      (value USB_B_Micro)
      (footprint digikey-footprints:USB_Micro_B_Female_10118193-0001LF)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6023BD96))
    (comp (ref J3)
      (value Conn_01x04)
      (footprint digikey-footprints:PinHeader_1x4_P2.54mm_Drill1.02mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x04) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6023E390))
    (comp (ref SW1)
      (value SW_SPDT_MSM)
      (footprint digikey-footprints:Toggle_Switch_100SP1T1B4M2QE)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPDT_MSM) (description "Switch, single pole double throw, center OFF position"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024D1C8))
    (comp (ref SW2)
      (value SW_SPDT_MSM)
      (footprint digikey-footprints:Toggle_Switch_100SP1T1B4M2QE)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPDT_MSM) (description "Switch, single pole double throw, center OFF position"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024DE6D))
    (comp (ref SW3)
      (value SW_SPDT_MSM)
      (footprint digikey-footprints:Toggle_Switch_100SP1T1B4M2QE)
      (datasheet ~)
      (libsource (lib Switch) (part SW_SPDT_MSM) (description "Switch, single pole double throw, center OFF position"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024E1D7))
    (comp (ref R2)
      (value 105E)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024E7D0))
    (comp (ref R1)
      (value 105E)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024F4D7))
    (comp (ref R3)
      (value 105E)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6024FF14))
    (comp (ref R6)
      (value 10K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6025CE8E))
    (comp (ref R5)
      (value 10K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6025DA85))
    (comp (ref R4)
      (value 10K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6025E6DF))
    (comp (ref R7)
      (value 10K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60299759))
    (comp (ref D2)
      (value LED)
      (footprint digikey-footprints:0805)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602A475E))
    (comp (ref D1)
      (value LED)
      (footprint digikey-footprints:0805)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602A57C9))
    (comp (ref R10)
      (value R)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 602AE2E0))
    (comp (ref R11)
      (value R)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 602AF25A))
    (comp (ref TP1)
      (value TestPoint)
      (footprint digikey-footprints:PC_TEST_POINT_SMD)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602E0E6F))
    (comp (ref R9)
      (value 1K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 602E1D33))
    (comp (ref Y1)
      (value 32Khz)
      (footprint digikey-footprints:Oscillator_XLH536025.000000I)
      (datasheet ~)
      (libsource (lib Device) (part Crystal) (description "Two pin crystal"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602F463F))
    (comp (ref C8)
      (value 100nF)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602F7127))
    (comp (ref C5)
      (value 100nF)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603022A1))
    (comp (ref C6)
      (value 100nF)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603026D2))
    (comp (ref C4)
      (value 1uF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part C_Polarized) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603063AF))
    (comp (ref U1)
      (value STM32L031K6Tx)
      (footprint digikey-footprints:QFN-32-1EP_5x5mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00140359.pdf)
      (libsource (lib MCU_ST_STM32L0) (part STM32L031K6Tx) (description "ARM Cortex-M0+ MCU, 32KB flash, 8KB RAM, 32MHz, 1.65-3.6V, 25 GPIO, LQFP-32"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6032319F))
    (comp (ref C2)
      (value 4,3pF)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603CA5B8))
    (comp (ref C3)
      (value 4,3pF)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603CB8C0))
    (comp (ref R8)
      (value 1M)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 603F8E75))
    (comp (ref R13)
      (value 100K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60403C7A))
    (comp (ref R12)
      (value 200K)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 6040529B))
    (comp (ref C7)
      (value 4,7uF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part C_Polarized) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6043A641))
    (comp (ref C1)
      (value 4,7uF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part C_Polarized) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60446C89))
    (comp (ref U3)
      (value LM3671MF-3.3)
      (footprint digikey-footprints:SOT-753)
      (datasheet http://www.ti.com/lit/ds/symlink/lm3670.pdf)
      (libsource (lib Regulator_Switching) (part LM3670MF) (description "Miniature Step-Down DC-DC Converter for Ultralow Voltage Circuits, 2.5V < Vin < 5.5V, adjustable output voltage, SOT-23-5"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604D4EA0))
    (comp (ref L1)
      (value 2,2uH)
      (footprint digikey-footprints:0805)
      (datasheet ~)
      (libsource (lib Device) (part L) (description Inductor))
      (sheetpath (names /) (tstamps /))
      (tstamp 604EE10C))
    (comp (ref C9)
      (value 4,7uF)
      (footprint Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B)
      (datasheet ~)
      (libsource (lib Device) (part C_Polarized) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60506A3D))
    (comp (ref S1)
      (value EG1218)
      (footprint MySymbols:slids_switch_spdt)
      (datasheet http://spec_sheets.e-switch.com/specs/P040040.pdf)
      (fields
        (field (name Category) Switches)
        (field (name DK_Datasheet_Link) http://spec_sheets.e-switch.com/specs/P040040.pdf)
        (field (name DK_Detail_Page) /product-detail/en/e-switch/EG1218/EG1903-ND/101726)
        (field (name Description) "SWITCH SLIDE SPDT 200MA 30V")
        (field (name Digi-Key_PN) EG1903-ND)
        (field (name Family) "Slide Switches")
        (field (name MPN) EG1218)
        (field (name Manufacturer) E-Switch)
        (field (name Status) Active))
      (libsource (lib dk_Slide-Switches) (part EG1218) (description "SWITCH SLIDE SPDT 200MA 30V"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602A1158))
    (comp (ref R14)
      (value R)
      (footprint digikey-footprints:0603)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 60310C7E)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x04)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Polarized)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Polarized))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal)
      (description "Two pin crystal")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_ST_STM32L0) (part STM32L031K4Tx)
      (aliases
        (alias STM32L031K6Tx))
      (description "ARM Cortex-M0+ MCU, 16KB flash, 8KB RAM, 32MHz, 1.65-3.6V, 25 GPIO, LQFP-32")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00140359.pdf)
      (footprints
        (fp LQFP*7x7mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32L031K4Tx)
        (field (name Footprint) Package_QFP:LQFP-32_7x7mm_P0.8mm))
      (pins
        (pin (num 1) (name VDD) (type power_in))
        (pin (num 2) (name PC14) (type BiDi))
        (pin (num 3) (name PC15) (type BiDi))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name PA0) (type BiDi))
        (pin (num 7) (name PA1) (type BiDi))
        (pin (num 8) (name PA2) (type BiDi))
        (pin (num 9) (name PA3) (type BiDi))
        (pin (num 10) (name PA4) (type BiDi))
        (pin (num 11) (name PA5) (type BiDi))
        (pin (num 12) (name PA6) (type BiDi))
        (pin (num 13) (name PA7) (type BiDi))
        (pin (num 14) (name PB0) (type BiDi))
        (pin (num 15) (name PB1) (type BiDi))
        (pin (num 16) (name VSS) (type power_in))
        (pin (num 17) (name VDD) (type power_in))
        (pin (num 18) (name PA8) (type BiDi))
        (pin (num 19) (name PA9) (type BiDi))
        (pin (num 20) (name PA10) (type BiDi))
        (pin (num 21) (name PA11) (type BiDi))
        (pin (num 22) (name PA12) (type BiDi))
        (pin (num 23) (name PA13) (type BiDi))
        (pin (num 24) (name PA14) (type BiDi))
        (pin (num 25) (name PA15) (type BiDi))
        (pin (num 26) (name PB3) (type BiDi))
        (pin (num 27) (name PB4) (type BiDi))
        (pin (num 28) (name PB5) (type BiDi))
        (pin (num 29) (name PB6) (type BiDi))
        (pin (num 30) (name PB7) (type BiDi))
        (pin (num 31) (name BOOT0) (type input))
        (pin (num 32) (name VSS) (type power_in))))
    (libpart (lib Regulator_Switching) (part ADP2108AUJ-1.0)
      (aliases
        (alias ADP2108AUJ-1.1)
        (alias ADP2108AUJ-1.2)
        (alias ADP2108AUJ-1.3)
        (alias ADP2108AUJ-1.5)
        (alias ADP2108AUJ-1.8)
        (alias ADP2108AUJ-1.82)
        (alias ADP2108AUJ-2.3)
        (alias ADP2108AUJ-2.5)
        (alias ADP2108AUJ-3.0)
        (alias ADP2108AUJ-3.3)
        (alias LM3670MF))
      (description "3MHz switching bucK regulator, 600mA 1.0V output voltage,")
      (docs https://www.analog.com/media/en/technical-documentation/data-sheets/ADP2108.pdf)
      (footprints
        (fp TSOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) ADP2108AUJ-1.0)
        (field (name Footprint) Package_TO_SOT_SMD:TSOT-23-5))
      (pins
        (pin (num 1) (name Vin) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name FB) (type input))
        (pin (num 5) (name SW) (type input))))
    (libpart (lib Switch) (part SW_SPDT_MSM)
      (description "Switch, single pole double throw, center OFF position")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_SPDT_MSM))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib dk_Barrel-Audio-Connectors) (part SJ1-3523N)
      (description "CONN JACK STEREO 3.5MM R/A")
      (docs https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
      (fields
        (field (name Reference) CON)
        (field (name Value) SJ1-3523N)
        (field (name Footprint) digikey-footprints:Headphone_Jack_3.5mm_SJ1-3523N)
        (field (name Datasheet) https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
        (field (name Digi-Key_PN) CP1-3523N-ND)
        (field (name MPN) SJ1-3523N)
        (field (name Category) "Connectors, Interconnects")
        (field (name Family) "Barrel - Audio Connectors")
        (field (name DK_Datasheet_Link) https://www.cui.com/product/resource/digikeypdf/sj1-352xn_series.pdf)
        (field (name DK_Detail_Page) /product-detail/en/cui-inc/SJ1-3523N/CP1-3523N-ND/738689)
        (field (name Description) "CONN JACK STEREO 3.5MM R/A")
        (field (name Manufacturer) "CUI Inc.")
        (field (name Status) Active))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name T) (type passive))
        (pin (num 3) (name R) (type passive))))
    (libpart (lib dk_PMIC-Battery-Chargers) (part MCP73832T-2ACI_OT)
      (description "IC LI-ION/LI-POLY CTRLR SOT23-5")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) MCP73832T-2ACI_OT)
        (field (name Footprint) digikey-footprints:SOT-753)
        (field (name Datasheet) http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
        (field (name Digi-Key_PN) MCP73832T-2ACI/OTCT-ND)
        (field (name MPN) MCP73832T-2ACI/OT)
        (field (name Category) "Integrated Circuits (ICs)")
        (field (name Family) "PMIC - Battery Chargers")
        (field (name DK_Datasheet_Link) http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
        (field (name DK_Detail_Page) /product-detail/en/microchip-technology/MCP73832T-2ACI-OT/MCP73832T-2ACI-OTCT-ND/1979805)
        (field (name Description) "IC LI-ION/LI-POLY CTRLR SOT23-5")
        (field (name Manufacturer) "Microchip Technology")
        (field (name Status) Active))
      (pins
        (pin (num 1) (name STAT) (type output))
        (pin (num 2) (name VSS) (type power_in))
        (pin (num 3) (name VBAT) (type power_out))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name PROG) (type input))))
    (libpart (lib dk_Slide-Switches) (part EG1218)
      (description "SWITCH SLIDE SPDT 200MA 30V")
      (docs http://spec_sheets.e-switch.com/specs/P040040.pdf)
      (fields
        (field (name Reference) S)
        (field (name Value) EG1218)
        (field (name Footprint) digikey-footprints:Switch_Slide_11.6x4mm_EG1218)
        (field (name Datasheet) http://spec_sheets.e-switch.com/specs/P040040.pdf)
        (field (name Digi-Key_PN) EG1903-ND)
        (field (name MPN) EG1218)
        (field (name Category) Switches)
        (field (name Family) "Slide Switches")
        (field (name DK_Datasheet_Link) http://spec_sheets.e-switch.com/specs/P040040.pdf)
        (field (name DK_Detail_Page) /product-detail/en/e-switch/EG1218/EG1903-ND/101726)
        (field (name Description) "SWITCH SLIDE SPDT 200MA 30V")
        (field (name Manufacturer) E-Switch)
        (field (name Status) Active))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/Connector.lib))
    (library (logical Connector_Generic)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/Connector_Generic.lib))
    (library (logical Device)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/Device.lib))
    (library (logical MCU_ST_STM32L0)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/MCU_ST_STM32L0.lib))
    (library (logical Regulator_Switching)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/Regulator_Switching.lib))
    (library (logical Switch)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/kicad-symbols/Switch.lib))
    (library (logical dk_Barrel-Audio-Connectors)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/digikey-kicad-library/digikey-symbols/dk_Barrel-Audio-Connectors.lib))
    (library (logical dk_PMIC-Battery-Chargers)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/digikey-kicad-library/digikey-symbols/dk_PMIC-Battery-Chargers.lib))
    (library (logical dk_Slide-Switches)
      (uri /Users/willemoldemans/Documents/PROJECTEN/libs/digikey-kicad-library/digikey-symbols/dk_Slide-Switches.lib)))
  (nets
    (net (code 1) (name "Net-(CON1-Pad2)")
      (node (ref CON1) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 2) (name "Net-(CON3-Pad2)")
      (node (ref R6) (pin 1))
      (node (ref CON3) (pin 2)))
    (net (code 3) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 4) (name +BATT)
      (node (ref U2) (pin 3))
      (node (ref S1) (pin 3))
      (node (ref J1) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 5) (name GND)
      (node (ref J2) (pin 6))
      (node (ref J3) (pin 4))
      (node (ref U3) (pin 2))
      (node (ref SW1) (pin 2))
      (node (ref SW2) (pin 2))
      (node (ref SW3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J2) (pin 5))
      (node (ref J2) (pin 4))
      (node (ref C7) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref U1) (pin 32))
      (node (ref U1) (pin 16))
      (node (ref C4) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref R7) (pin 2)))
    (net (code 6) (name "Net-(J2-Pad2)")
      (node (ref J2) (pin 2)))
    (net (code 7) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3)))
    (net (code 8) (name "Net-(CON2-Pad1)")
      (node (ref CON2) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 9) (name "Net-(CON1-Pad1)")
      (node (ref CON1) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 10) (name "Net-(CON3-Pad1)")
      (node (ref CON3) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 11) (name LED1)
      (node (ref U1) (pin 14))
      (node (ref R1) (pin 2)))
    (net (code 12) (name LED2)
      (node (ref U1) (pin 30))
      (node (ref R2) (pin 1)))
    (net (code 13) (name LED3)
      (node (ref U1) (pin 29))
      (node (ref R3) (pin 2)))
    (net (code 14) (name "Net-(CON2-Pad2)")
      (node (ref CON2) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 15) (name DET2)
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 11)))
    (net (code 16) (name DET1)
      (node (ref U1) (pin 12))
      (node (ref R4) (pin 2)))
    (net (code 17) (name DET3)
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 10)))
    (net (code 18) (name SWITCH12)
      (node (ref SW1) (pin 3))
      (node (ref U1) (pin 8)))
    (net (code 19) (name SWITCH2)
      (node (ref SW2) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 20) (name SWITCH22)
      (node (ref SW2) (pin 3))
      (node (ref U1) (pin 9)))
    (net (code 21) (name SWITCH3)
      (node (ref SW3) (pin 1))
      (node (ref U1) (pin 28)))
    (net (code 22) (name SWITCH32)
      (node (ref SW3) (pin 3))
      (node (ref U1) (pin 27)))
    (net (code 23) (name "Net-(D1-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 24) (name VBUS)
      (node (ref J2) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref C1) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref R14) (pin 2)))
    (net (code 25) (name "Net-(D2-Pad2)")
      (node (ref R11) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 26) (name "Net-(R11-Pad2)")
      (node (ref R11) (pin 2))
      (node (ref U2) (pin 1)))
    (net (code 27) (name RST)
      (node (ref U1) (pin 4))
      (node (ref TP1) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 28) (name BOOT0)
      (node (ref U1) (pin 31)))
    (net (code 29) (name "Net-(U1-Pad20)")
      (node (ref U1) (pin 20)))
    (net (code 30) (name "Net-(U1-Pad21)")
      (node (ref U1) (pin 21)))
    (net (code 31) (name "Net-(U1-Pad22)")
      (node (ref U1) (pin 22)))
    (net (code 32) (name SWDIO)
      (node (ref U1) (pin 23))
      (node (ref J3) (pin 2)))
    (net (code 33) (name SWCLK)
      (node (ref U1) (pin 24))
      (node (ref J3) (pin 3)))
    (net (code 34) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 35) (name SWITCH1)
      (node (ref U1) (pin 13))
      (node (ref SW1) (pin 1)))
    (net (code 36) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 37) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 38) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 39) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 40) (name +3V3)
      (node (ref L1) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref CON3) (pin 3))
      (node (ref U3) (pin 4))
      (node (ref CON2) (pin 3))
      (node (ref CON1) (pin 3))
      (node (ref C4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref U1) (pin 5))
      (node (ref U1) (pin 17))
      (node (ref U1) (pin 1))
      (node (ref C6) (pin 1)))
    (net (code 41) (name "Net-(C2-Pad1)")
      (node (ref Y1) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 42) (name "Net-(C3-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref C3) (pin 1))
      (node (ref R8) (pin 2)))
    (net (code 43) (name MEAS_VBATT)
      (node (ref R13) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 44) (name "Net-(L1-Pad1)")
      (node (ref L1) (pin 1))
      (node (ref U3) (pin 5)))
    (net (code 45) (name +BATT_SWITCHED)
      (node (ref S1) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 1)))
    (net (code 46) (name "Net-(R14-Pad1)")
      (node (ref S1) (pin 1))
      (node (ref R14) (pin 1)))))